(footprint "L_Wuerth_WE-PDF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded Power Inductor, Wuerth Elektronik, WE-PDF, SMD, https://katalog.we-online.de/pbs/datasheet/7447797022.pdf")
	(tags "Choke Shielded Power Inductor WE-PDF Wuerth")
	(property "Reference" "REF**"
		(at 0 -6.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wuerth_WE-PDF"
		(at 0.1 6.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.1 0)
		(size 2.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.1 0)
		(size 2.4 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Wuerth_WE-PDF.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
