(footprint "L_Wurth_WE-LQSH-2010"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Semi-Shielded High Saturation Power Inductor, body 2x1.6mm, https://www.we-online.com/catalog/en/WE-LQSH#/articles/WE-LQSH-2010")
	(tags "SMT")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wurth_WE-LQSH-2010"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.8 0)
		(size 0.8 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.8 0)
		(size 0.8 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD_Wurth.3dshapes/L_Wurth_WE-LQSH-2010.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
