(footprint "L_Axial_L17.5mm_D12.0mm_P7.62mm_Vertical_Vishay_IM-10-46"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Axial series, Axial, Vertical, pin pitch=7.62mm, , length*diameter=17.5*12mm^2, Vishay, IM-10-46, http://www.vishay.com/docs/34030/im10.pdf")
	(tags "Inductor Axial series Axial Vertical pin pitch 7.62mm  length 17.5mm diameter 12mm Vishay IM-10-46")
	(property "Reference" "REF**"
		(at 3.81 -7.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Axial_L17.5mm_D12.0mm_P7.62mm_Vertical_Vishay_IM-10-46"
		(at 3.81 7.12 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 7.62 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L17.5mm_D12.0mm_P7.62mm_Vertical_Vishay_IM-10-46.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
