(footprint "L_Axial_L24.0mm_D7.1mm_P5.08mm_Vertical_Vishay_IM-10-28"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Axial series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=24*7.1mm^2, Vishay, IM-10-28, http://www.vishay.com/docs/34035/im10.pdf")
	(tags "Inductor Axial series Axial Vertical pin pitch 5.08mm  length 24mm diameter 7.1mm Vishay IM-10-28")
	(property "Reference" "REF**"
		(at 2.54 -4.67 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Axial_L24.0mm_D7.1mm_P5.08mm_Vertical_Vishay_IM-10-28"
		(at 2.54 4.67 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5.08 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L24.0mm_D7.1mm_P5.08mm_Vertical_Vishay_IM-10-28.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
