(footprint "L_Axial_L5.3mm_D2.2mm_P2.54mm_Vertical_Vishay_IM-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor, Axial series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.3*2.2mm^2, Vishay, IM-1, http://www.vishay.com/docs/34030/im.pdf")
	(tags "Inductor Axial series Axial Vertical pin pitch 2.54mm  length 5.3mm diameter 2.2mm Vishay IM-1")
	(property "Reference" "REF**"
		(at 1.27 -2.22 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Axial_L5.3mm_D2.2mm_P2.54mm_Vertical_Vishay_IM-1"
		(at 1.27 2.22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.27 -2.22 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L5.3mm_D2.2mm_P2.54mm_Vertical_Vishay_IM-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
