(footprint "L_CommonMode_TDK_B82746S6702A040"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8A, 3Phase, Triple Coil, CM Choke, https://www.tdk-electronics.tdk.com/inf/30/ds/b82746s.pdf")
	(tags "common mode filter triple choke")
	(property "Reference" "REF**"
		(at 1.918584 -10.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_TDK_B82746S6702A040"
		(at 20 39 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 19.918584 11.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 150)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 19.918584 34.5 20)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 39.837168 0 260)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 26.4718 16.088611 52)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 12.668122 14.880946 292)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 20.61583 3.530442 172)
		(size 2.5 2.5)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_TDK_B82746S6702A040.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
