(footprint "L_CommonMode_TDK_B82747E6353A040"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "35A, 3Phase, Triple Coil, CM Choke, drill hole 3mm ( https://product.tdk.com/system/files/dam/doc/product/emc/emc/line-filter/data_sheet/30/ds/b82747e6.pdf )")
	(tags "three phase common mode triple choke")
	(property "Reference" "REF**"
		(at -2.2 -14.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_TDK_B82747E6353A040"
		(at 15.5 54 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 15.9 19.1 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 20 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 40 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 31 40 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31 20 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 31 0 90)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_TDK_B82747E6353A040.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
