(footprint "L_CommonMode_VAC_T60405-S6123-X140"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "40A, 3Phase, Triple Coil, CM Choke, https://vacuumschmelze.com/03_Documents/Datasheets%20-%20Drawings/Commom-Mode-Chokes/6123-X140.pdf")
	(tags "common mode filter")
	(property "Reference" "REF**"
		(at -16.526008 -26.552412 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_VAC_T60405-S6123-X140"
		(at 3.173992 20.992692 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.169637 -6.797308 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 335)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at -19.52962 -12.879556)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -1.132186 -12.940948 250)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 19.786646 -23.414317)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.641097 -7.450976)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 9.251885 15.901949)
		(size 5.7 5.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_VAC_T60405-S6123-X140.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
