(footprint "L_CommonMode_VAC_T60405-S6123-X402"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "30A, 3Phase N, Quadruple Coil, CM Choke, https://vacuumschmelze.com/03_Documents/Datasheets%20-%20Drawings/Commom-Mode-Chokes/6123-X402.pdf")
	(tags "common mode filter quadruple choke")
	(property "Reference" "REF**"
		(at -7.5 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_VAC_T60405-S6123-X402"
		(at 18.73833 50.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 18.73833 18.73833 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 45)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 10.189886 16.447781 60)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 37.47666 0 315)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.028879 10.189886 330)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 37.47666 37.47666 225)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 27.286774 21.028879 240)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 37.47666 135)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 16.447781 27.286774 150)
		(size 5.5 5.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_VAC_T60405-S6123-X402.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
