(footprint "L_CommonMode_Wuerth_WE-CMB-L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wuerth, WE-CMB, Bauform L,")
	(tags "CommonModeChoke Gleichtaktdrossel ")
	(property "Reference" "REF**"
		(at 6 -10 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_Wuerth_WE-CMB-L"
		(at 6 20.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "2"
		(at 2.5 0 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 6 5 0)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 9.5 10 0)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 9.5 0 0)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 2.5 10 0)
		(layer "F.Fab")
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 10)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 12 10)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 12 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_Wuerth_WE-CMB-L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
