(footprint "L_CommonMode_Wuerth_WE-CMB-M"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wuerth, WE-CMB, Bauform M,")
	(tags "CommonModeChoke Gleichtaktdrossel ")
	(property "Reference" "REF**"
		(at 5.35 -8.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_CommonMode_Wuerth_WE-CMB-M"
		(at 5.35 16.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "2"
		(at 7.85 0.25 0)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at 2.85 0.25 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 5.35 3.75 0)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 2.85 7.75 0)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 7.85 7.75 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10.7 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.7 7.5)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.5)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_CommonMode_Wuerth_WE-CMB-M.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
