(footprint "L_Toroid_Vertical_L16.0mm_W8.0mm_P7.62mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "L_Toroid, Vertical series, Radial, pin pitch=7.62mm, , length*width=16*8mm^2")
	(tags "L_Toroid Vertical series Radial pin pitch 7.62mm  length 16mm width 8mm")
	(property "Reference" "REF**"
		(at 0 -2.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "L_Toroid_Vertical_L16.0mm_W8.0mm_P7.62mm"
		(at 0 10.37 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 7.62)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Toroid_Vertical_L16.0mm_W8.0mm_P7.62mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
