(footprint "L_Wurth_WE-HCFT-3521"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded High Current Inductor, body 21.5x36mm, https://www.we-online.com/catalog/en/WE-HCFT#/articles/WE-HCFT-3521")
	(tags "THT")
	(property "Reference" "REF**"
		(at 4.45 -12.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "L_Wurth_WE-HCFT-3521"
		(at 4.45 26.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.45 6.75 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 0 13.5)
		(size 3.75 3.75)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 8.9 0)
		(size 3.75 3.75)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 5 10)
		(drill oval 3 8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 8.9 13.5)
		(size 5 10)
		(drill oval 3 8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_THT_Wurth.3dshapes/L_Wurth_WE-HCFT-3521.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
