(footprint "SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
	(tags "solder jumper open")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(at 0 1.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(pad "1" smd rect
		(at -0.65 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 0.65 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
