(footprint "SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm_NumberLabels"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
	(tags "net tie solder jumper bridged")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm_NumberLabels"
		(at 0 1.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(net_tie_pad_groups "1, 2")
	(fp_text user "3"
		(at 2.6 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -2.6 0 0)
		(layer "F.SilkS")
	)
	(pad "1" smd rect
		(at -1.3 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 0 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 1.3 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
