(footprint "SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
	(tags "net tie solder jumper bridged")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm"
		(at 0 1.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(net_tie_pad_groups "1,2")
	(pad "1" smd custom
		(at -1.3 0)
		(size 1 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.25)
				(end 0.5 0.25)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0 -0.25)
				(end 0.5 -0.25)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.55 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.55 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at 0 0)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd custom
		(at 1.3 0)
		(size 1 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.25)
				(end 0.5 0.25)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0 -0.25)
				(end 0.5 -0.25)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0 0.75) (xy -0.55 0.75) (xy -0.55 -0.75) (xy 0 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
)
