(footprint "LED_1W_3W_R8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.gme.cz/data/attachments/dsh.518-234.1.pdf")
	(tags "LED 1W 3W 5W")
	(property "Reference" "REF**"
		(at -5.08 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_1W_3W_R8"
		(at 0 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.35 1.35)
		(size 3.5 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 6.35 -1.35)
		(size 3.5 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd circle
		(at 0 0)
		(size 5.7 5.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1W_3W_R8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
