(footprint "LED_Cree-PLCC6_4.7x1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4.7mm x 1.5mm PLCC6 LED, http://www.cree.com/led-components/media/documents/1381-QLS6AFKW.pdf")
	(tags "LED Cree PLCC-6")
	(property "Reference" "REF**"
		(at 0 1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Cree-PLCC6_4.7x1.5mm"
		(at 0 3.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.8 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.02 0.335)
		(size 0.66 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.21 -0.25)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.53 -0.25)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.53 -0.25)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.21 -0.25)
		(size 0.4 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.02 0.335)
		(size 0.66 0.63)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Cree-PLCC6_4.7x1.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
