(footprint "LED_Cree-XH"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds-XHB.pdf")
	(tags "LED Cree XH")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Cree-XH"
		(at 0 2.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.65 -0.75)
		(size 1.35 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.65 0.75)
		(size 1.35 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1 -0.75)
		(size 0.7 1.2)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1 0.75)
		(size 0.7 1.2)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.5 0)
		(size 0.5 0.33)
		(layers "F.Cu" "F.Mask")
	)
	(pad "1" smd rect
		(at -0.65 0)
		(size 1.7 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 1.1 0)
		(size 0.8 3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 1.5 0)
		(size 0.5 0.33)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Cree-XH.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
