(footprint "LED_Cree-XHP50_12V"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Cree XHP50, 12V footprint, http://www.cree.com/~/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP50.pdf")
	(tags "LED XHP50 Cree")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Cree-XHP50_12V"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.14 -1.32)
		(size 0.5 2.14)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.61 -1.575)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.61 -0.525)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.61 0.525)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.61 1.575)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.61 -1.575)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.61 -0.525)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.61 0.525)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.61 1.575)
		(size 0.97 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 2.14 1.32)
		(size 0.5 2.14)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.14 1.32)
		(size 0.5 2.14)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.14 -1.32)
		(size 0.5 2.14)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.89 -1.32)
		(size 1 2.14)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 0 0)
		(size 2.78 4.78)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 1.89 1.32)
		(size 1 2.14)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes\\LED_Cree-XHP50_12V.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
