(footprint "LED_Everlight-SMD3528_3.5x2.8mm_67-21ST"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3.5mm x 2.8mm mid-power LED, https://www.everlight.com/wp-content/plugins/ItemRelationship/product_files/pdf/DSE-0020730-67-21ST-KK6C-HXXXX96Z6-2T_V3.pdf")
	(tags "LED 3528")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Everlight-SMD3528_3.5x2.8mm_67-21ST"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.34 0)
		(size 1.1 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "2" smd roundrect
		(at 0.81 0)
		(size 2.1 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Everlight-SMD3528_3.5x2.8mm_67-21ST.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
