(footprint "LED_Kingbright_APHBM2012_2x1.25mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Dual LED SMD https://www.kingbrightusa.com/KCpack.asp?txtPack=APHBM2012")
	(tags "LED Kingbright APHM2012")
	(property "Reference" "REF**"
		(at 0.15 -2.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Kingbright_APHBM2012_2x1.25mm"
		(at -0.05 2.6 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.15 -2.5 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.475 -0.9 90)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.475 0.9 90)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.475 0.9 90)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.475 -0.9 90)
		(size 1.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_APHBM2012_2x1.25mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
