(footprint "LED_Kingbright_KPA-3010_3x2x1mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Kingbright surface mount LED, right angle, 3.0 x 2.0 x 1.0 mm, https://www.kingbright.com/attachments/file/psearch/000/00/00/KPA-3010SURCK(Ver.26A).pdf")
	(tags "Kingbright LED right-angle")
	(property "Reference" "REF**"
		(at 0 2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Kingbright_KPA-3010_3x2x1mm"
		(at 0 3.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.75 0.5)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "2" smd roundrect
		(at 1.75 0.5)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "3" smd roundrect
		(at 0 1.15)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_KPA-3010_3x2x1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
