(footprint "LED_Kingbright_KPBD-3224"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Kingbright, dual LED, red-green, dome lens, 3.2 x 2.4 mm Surface Mount LED Lamp (https://docs.rs-online.com/b881/0900766b81396b45.pdf)")
	(tags "Kingbright dual LED KPBD-3224")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Kingbright_KPBD-3224"
		(at 0 4.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "1"
		(at -1.6 -2.15 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -0.05 -0.05 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.7 -1.6 270)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -0.7 1.6 270)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at 0.7 -1.6 270)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at 0.7 1.6 270)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_KPBD-3224.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
