(footprint "LED_LiteOn_LTST-C235KGKRKT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "downfacing reverse mount led, https://optoelectronics.liteon.com/upload/download/DS22-2009-0219/LTST-C235KGKRKT.pdf")
	(tags "LED reverse down facing")
	(property "Reference" "REF**"
		(at 0 2.44 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_LiteOn_LTST-C235KGKRKT"
		(at 0.1 -2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at 0 0)
		(size 2.1 2.8)
		(drill oval 2.1 2.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.9 -0.5 180)
		(size 1.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 1.9 -0.5 180)
		(size 1.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1.9 0.5 180)
		(size 1.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9 0.5 180)
		(size 1.3 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_LiteOn_LTST-C235KGKRKT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
