(footprint "LED_LiteOn_LTST-C295K_1.6x0.8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Topview dual http://optoelectronics.liteon.com/upload/download/DS22-2009-0072/LTST-C295KGKRKT.PDF")
	(tags "SMD Top view Dual colour")
	(property "Reference" "REF**"
		(at 0 -1.45 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "LED_LiteOn_LTST-C295K_1.6x0.8mm"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.6 -0.35 90)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.6 0.35 90)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.6 -0.35 90)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.6 0.35 90)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_LiteOn_LTST-C295K_1.6x0.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
