(footprint "LED_OPSCO_SK6812_PLCC4_5.0x5.0mm_P3.1mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5.0mm x 5.0mm Addressable RGB LED,  https://www.lcsc.com/datasheet/lcsc_datasheet_2303300930_OPSCO-Optoelectronics-SK6812-B_C5380881.pdf#page=5")
	(tags "LED RGB NeoPixel Serial PLCC-4 5050")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_OPSCO_SK6812_PLCC4_5.0x5.0mm_P3.1mm"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "1"
		(at -4.225 -1.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.55 -1.6)
		(size 1.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at -2.55 1.6)
		(size 1.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at 2.55 1.6)
		(size 1.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at 2.55 -1.6)
		(size 1.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_OPSCO_SK6812_PLCC4_5.0x5.0mm_P3.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
