(footprint "LED_Osram_Lx_P47F_D2mm_ReverseMount"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "OSRAM, reverse-mount LED, SMD, 2mm diameter, http://www.farnell.com/datasheets/2711587.pdf")
	(tags "LED ReverseMount Reverse")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_Osram_Lx_P47F_D2mm_ReverseMount"
		(at 0 2.425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -1.55 0.375)
		(size 0.5 0.7)
		(layers "F.Mask" "F.Paste")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 2.1 2.1)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd rect
		(at 1.55 -0.375)
		(size 0.5 0.7)
		(layers "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -2.3 0)
		(size 2 2.5)
		(layers "F.Cu")
	)
	(pad "2" smd rect
		(at 2.3 0)
		(size 2 2.5)
		(layers "F.Cu")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Osram_Lx_P47F_D2mm_ReverseMount.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
