(footprint "LED_RGB_Cree-PLCC-6_6x5mm_P2.1mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.farnell.com/datasheets/2003905.pdf")
	(tags "LED RGB PLCC-6 CLP6C-FBK")
	(property "Reference" "REF**"
		(at 0 -3.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_RGB_Cree-PLCC-6_6x5mm_P2.1mm"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.1 0.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.45 -2.1)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.45 0)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.45 2.1)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.45 2.1)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.45 0)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.45 -2.1)
		(size 2.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_Cree-PLCC-6_6x5mm_P2.1mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
