(footprint "LED_RGB_Everlight_EASV3015RGBA0_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LED, RGB, right-angle, clear, https://everlightamericas.com/index.php?controller=attachment&id_attachment=3220")
	(tags "LED RGB right-angle")
	(property "Reference" "REF**"
		(at 0 1.87 180)
		(layer "F.SilkS")
	)
	(property "Value" "LED_RGB_Everlight_EASV3015RGBA0_Horizontal"
		(at 0 -1.72 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.425 -0.53)
		(size 0.55 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.425 -0.75)
		(size 0.55 0.34)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.425 -0.75)
		(size 0.55 0.34)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.425 -0.53)
		(size 0.55 0.78)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_Everlight_EASV3015RGBA0_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
