(footprint "LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3.5mm x 3.5mm PLCC4 Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf")
	(tags "LED RGB NeoPixel Mini PLCC-4 3535")
	(property "Reference" "REF**"
		(at 0 -2.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "1"
		(at -3.2 -0.875 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.75 -0.875)
		(size 1.6 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.75 0.875)
		(size 1.6 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.75 0.875)
		(size 1.6 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.75 -0.875)
		(size 1.6 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
