(footprint "LED_BL-FL7680RGB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "'Piranha' RGB LED, through hole, common anode, 7.62x7.62mm, BGRA pin order, https://cdn-shop.adafruit.com/datasheets/BL-FL7680RGB.pdf")
	(tags "RGB LED Piranha Super-Flux BetLux")
	(property "Reference" "REF**"
		(at 2.54 -2.27 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_BL-FL7680RGB"
		(at 2.54 7.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 2.54 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5.08)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 5.08)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.08 0)
		(size 2.35 2.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_BL-FL7680RGB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
