(footprint "LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRGrey"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "LED, diameter 3.0mm, horizontal offset 1.27mm, z-position of LED center 2.0mm, 2 pins, infrared, grey, generated by kicad-footprint-generator")
	(tags "LED IR")
	(property "Reference" "REF**"
		(at 1.27 -1.96 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRGrey"
		(at 1.27 7.63 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.27 3.12 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm_IRGrey.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
