(footprint "LED_VCCLite_5381H3_6.35x6.35mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Amber 5381 Series LED VCCLite https://vcclite.com/wp-content/uploads/wpallimport/files/files/5381Series.pdf http://static.vcclite.com/pdf/Mounting%20Hole%20Pattern%202.pdf")
	(tags "Amber 5381 Series LED")
	(property "Reference" "REF**"
		(at -1 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "LED_VCCLite_5381H3_6.35x6.35mm"
		(at 1.27 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.27 1.27 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 1.75 1.75)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 2.54 270)
		(size 1.75 1.75)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_VCCLite_5381H3_6.35x6.35mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
