(footprint "A20_OLINUXINO_LIME2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "A20 Olinuxino LIME2, 1.2GHz, 512-1024MB RAM, Micro-SD, NAND or eMMC, 1000Mbit Ethernet")
	(tags "A20 Olimex Olinuxino LIME2 development board")
	(property "Reference" "REF**"
		(at 2 -31 0)
		(layer "F.SilkS")
	)
	(property "Value" "A20_OLINUXINO_LIME2"
		(at 3.77 31.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "GPIO-3"
		(at 20.05 22.68 0)
		(layer "F.SilkS")
	)
	(fp_text user "GPIO-4"
		(at -24.3 -25.35 90)
		(layer "F.SilkS")
	)
	(fp_text user "LCD_CON"
		(at 19.85 -22.63 0)
		(layer "F.SilkS")
	)
	(fp_text user "GPIO-1"
		(at -1.03 -16 0)
		(layer "F.SilkS")
	)
	(fp_text user "GPIO-2"
		(at -5.44 16.31 0)
		(layer "F.SilkS")
	)
	(fp_text user "Cutout"
		(at -30.08 3.19 0)
		(layer "Dwgs.User")
	)
	(fp_text user " for shield"
		(at -1.2 -2.2 0)
		(layer "Dwgs.User")
	)
	(fp_text user "required"
		(at 37.92 -11.81 0)
		(layer "Dwgs.User")
	)
	(fp_text user "required"
		(at -30.08 5.19 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Cut out >=22x22mm"
		(at 3.52 5.29 0)
		(layer "Dwgs.User")
	)
	(fp_text user "CPU 18mmx18mm"
		(at 2.2 -5.8 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Mininum cut out "
		(at 2 -4 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Cutout"
		(at 37.92 -13.81 0)
		(layer "Dwgs.User")
	)
	(fp_text user " 20mm heatsink"
		(at 0.92 9.09 0)
		(layer "Dwgs.User")
	)
	(fp_text user "if using"
		(at -1.58 7.19 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -20.13 -28.19)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -20.13 -18.04)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.32 -20.19)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.32 20.45)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.33 -26.54)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.33 26.8)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 14.54 -20.19)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 14.54 20.45)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 21.53 -26.54)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 21.53 26.8)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1-1" smd rect
		(at -8.95 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-2" smd rect
		(at -8.95 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-3" smd rect
		(at -7.68 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-4" smd rect
		(at -7.68 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-5" smd rect
		(at -6.41 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-6" smd rect
		(at -6.41 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-7" smd rect
		(at -5.14 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-8" smd rect
		(at -5.14 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-9" smd rect
		(at -3.87 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-10" smd rect
		(at -3.87 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-11" smd rect
		(at -2.6 -18.16 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-12" smd rect
		(at -2.6 -22.23 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-13" smd rect
		(at -1.33 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-14" smd rect
		(at -1.33 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-15" smd rect
		(at -0.06 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-16" smd rect
		(at -0.06 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-17" smd rect
		(at 1.21 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-18" smd rect
		(at 1.21 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-19" smd rect
		(at 2.48 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-20" smd rect
		(at 2.48 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-21" smd rect
		(at 3.75 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-22" smd rect
		(at 3.75 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-23" smd rect
		(at 5.02 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-24" smd rect
		(at 5.02 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-25" smd rect
		(at 6.29 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-26" smd rect
		(at 6.29 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-27" smd rect
		(at 7.56 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-28" smd rect
		(at 7.56 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-29" smd rect
		(at 8.83 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-30" smd rect
		(at 8.83 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-31" smd rect
		(at 10.09 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-32" smd rect
		(at 10.09 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-33" smd rect
		(at 11.37 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-34" smd rect
		(at 11.37 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-35" smd rect
		(at 12.64 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-36" smd rect
		(at 12.64 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-37" smd rect
		(at 13.91 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-38" smd rect
		(at 13.91 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-39" smd rect
		(at 15.18 -18.16 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1-40" smd rect
		(at 15.18 -22.23 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-1" smd rect
		(at -8.95 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-2" smd rect
		(at -8.95 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-3" smd rect
		(at -7.68 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-4" smd rect
		(at -7.68 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-5" smd rect
		(at -6.41 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-6" smd rect
		(at -6.41 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-7" smd rect
		(at -5.14 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-8" smd rect
		(at -5.14 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-9" smd rect
		(at -3.87 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-10" smd rect
		(at -3.87 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-11" smd rect
		(at -2.6 22.48 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-12" smd rect
		(at -2.6 18.42 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-13" smd rect
		(at -1.33 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-14" smd rect
		(at -1.33 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-15" smd rect
		(at -0.06 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-16" smd rect
		(at -0.06 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-17" smd rect
		(at 1.21 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-18" smd rect
		(at 1.21 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-19" smd rect
		(at 2.48 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-20" smd rect
		(at 2.48 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-21" smd rect
		(at 3.75 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-22" smd rect
		(at 3.75 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-23" smd rect
		(at 5.02 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-24" smd rect
		(at 5.02 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-25" smd rect
		(at 6.29 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-26" smd rect
		(at 6.29 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-27" smd rect
		(at 7.56 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-28" smd rect
		(at 7.56 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-29" smd rect
		(at 8.83 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-30" smd rect
		(at 8.83 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-31" smd rect
		(at 10.09 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-32" smd rect
		(at 10.09 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-33" smd rect
		(at 11.37 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-34" smd rect
		(at 11.37 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-35" smd rect
		(at 12.64 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-36" smd rect
		(at 12.64 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-37" smd rect
		(at 13.91 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-38" smd rect
		(at 13.91 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-39" smd rect
		(at 15.18 22.48 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2-40" smd rect
		(at 15.18 18.42 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-1" smd rect
		(at -1.97 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-2" smd rect
		(at -1.97 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-3" smd rect
		(at -0.7 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-4" smd rect
		(at -0.7 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-5" smd rect
		(at 0.57 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-6" smd rect
		(at 0.57 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-7" smd rect
		(at 1.84 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-8" smd rect
		(at 1.84 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-9" smd rect
		(at 3.11 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-10" smd rect
		(at 3.11 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-11" smd rect
		(at 4.38 28.83 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-12" smd rect
		(at 4.38 24.76 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-13" smd rect
		(at 5.65 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-14" smd rect
		(at 5.65 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-15" smd rect
		(at 6.92 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-16" smd rect
		(at 6.92 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-17" smd rect
		(at 8.19 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-18" smd rect
		(at 8.19 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-19" smd rect
		(at 9.46 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-20" smd rect
		(at 9.46 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-21" smd rect
		(at 10.73 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-22" smd rect
		(at 10.73 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-23" smd rect
		(at 12 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-24" smd rect
		(at 12 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-25" smd rect
		(at 13.27 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-26" smd rect
		(at 13.27 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-27" smd rect
		(at 14.54 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-28" smd rect
		(at 14.54 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-29" smd rect
		(at 15.81 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-30" smd rect
		(at 15.81 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-31" smd rect
		(at 17.08 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-32" smd rect
		(at 17.08 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-33" smd rect
		(at 18.35 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-34" smd rect
		(at 18.35 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-35" smd rect
		(at 19.62 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-36" smd rect
		(at 19.62 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-37" smd rect
		(at 20.89 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-38" smd rect
		(at 20.89 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-39" smd rect
		(at 22.16 28.83 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3-40" smd rect
		(at 22.16 24.76 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-1" smd rect
		(at -18.1 -17.4 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-2" smd rect
		(at -22.16 -17.4 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-3" smd rect
		(at -18.1 -18.67 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-4" smd rect
		(at -22.16 -18.67 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-5" smd rect
		(at -18.1 -19.94 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-6" smd rect
		(at -22.16 -19.94 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-7" smd rect
		(at -18.1 -21.21 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-8" smd rect
		(at -22.16 -21.21 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-9" smd rect
		(at -18.1 -22.48 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-10" smd rect
		(at -22.16 -22.48 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-11" smd rect
		(at -18.1 -23.75 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-12" smd rect
		(at -22.16 -23.75 180)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-13" smd rect
		(at -18.1 -25.02)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-14" smd rect
		(at -22.16 -25.02)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-15" smd rect
		(at -18.1 -26.29)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-16" smd rect
		(at -22.16 -26.29)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-17" smd rect
		(at -18.1 -27.56)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-18" smd rect
		(at -22.16 -27.56)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-19" smd rect
		(at -18.1 -28.83)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4-20" smd rect
		(at -22.16 -28.83)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-1" smd rect
		(at -1.97 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-2" smd rect
		(at -1.97 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-3" smd rect
		(at -0.7 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-4" smd rect
		(at -0.7 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-5" smd rect
		(at 0.57 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-6" smd rect
		(at 0.57 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-7" smd rect
		(at 1.84 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-8" smd rect
		(at 1.84 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-9" smd rect
		(at 3.11 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-10" smd rect
		(at 3.11 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-11" smd rect
		(at 4.38 -24.51 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-12" smd rect
		(at 4.38 -28.58 90)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-13" smd rect
		(at 5.65 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-14" smd rect
		(at 5.65 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-15" smd rect
		(at 6.92 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-16" smd rect
		(at 6.92 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-17" smd rect
		(at 8.19 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-18" smd rect
		(at 8.19 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-19" smd rect
		(at 9.46 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-20" smd rect
		(at 9.46 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-21" smd rect
		(at 10.73 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-22" smd rect
		(at 10.73 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-23" smd rect
		(at 12 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-24" smd rect
		(at 12 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-25" smd rect
		(at 13.27 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-26" smd rect
		(at 13.27 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-27" smd rect
		(at 14.54 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-28" smd rect
		(at 14.54 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-29" smd rect
		(at 15.81 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-30" smd rect
		(at 15.81 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-31" smd rect
		(at 17.08 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-32" smd rect
		(at 17.08 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-33" smd rect
		(at 18.35 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-34" smd rect
		(at 18.35 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-35" smd rect
		(at 19.62 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-36" smd rect
		(at 19.62 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-37" smd rect
		(at 20.89 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-38" smd rect
		(at 20.89 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-39" smd rect
		(at 22.16 -24.51 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D-40" smd rect
		(at 22.16 -28.58 270)
		(size 1.8 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/A20_OLINUXINO_LIME2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
