(footprint "Adafruit_Feather_32u4_RFM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Footprint for the Adafruit Feather 32u4 RFM series of boards, https://learn.adafruit.com/adafruit-feather-32u4-radio-with-rfm69hcw-module")
	(tags "Adafruit Feather 32u4 RFM")
	(property "Reference" "REF**"
		(at 10.16 -7.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "Adafruit_Feather_32u4_RFM"
		(at 10.16 45.72 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10.16 19.05 270)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15625)
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 0 7.62)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0 10.16)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 0 12.7)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 0 15.24)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 0 17.78)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 0 20.32)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 0 22.86)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 0 25.4)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 0 27.94)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 0 30.48)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 0 33.02)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 0 35.56)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 0 38.1)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at 20.32 38.1 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at 20.32 35.56 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at 20.32 33.02 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at 20.32 30.48 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 20.32 27.94 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 20.32 25.4 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 20.32 22.86 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 20.32 20.32 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 20.32 17.78 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 20.32 15.24 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 20.32 12.7 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 20.32 10.16 180)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole oval
		(at 3.81 43.18 90)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole oval
		(at 11.43 43.18 90)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole oval
		(at 13.97 43.18 90)
		(size 2.6 1.6)
		(drill 1
			(offset 0.3 0)
		)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather_32u4_RFM.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
