(footprint "Carambola2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8devices Carambola2, OpenWRT, industrial SoM computer, https://www.8devices.com/media/products/carambola2/downloads/carambola2-datasheet.pdf")
	(tags "carambola2 8devices")
	(property "Reference" "REF**"
		(at 0 -20.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Carambola2"
		(at -0.5 21.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -13.5 -17 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -15 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -13 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -9 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -7 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -5 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -3 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 -1 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 1 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 3 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 5 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 7 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 9 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 11 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 15 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.5 17 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.45 -11 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -13.45 13 180)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -10 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -10 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -8 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -8 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -6 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -6 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -4 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -4 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -2 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 6 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 6 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 8 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 8 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.25 0.57) (xy 0.1 0.57) (xy 0.1 -0.58) (xy 1.25 -0.58)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 10 -18.5 90)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 10 18.5 270)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -17)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -15)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -13)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -11)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -9)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -7)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -5)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -3)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 -1)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 1)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 3)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 5)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 7)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 9)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 11)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 13)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 15)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 13.5 17)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.27 0.45) (xy -0.01 0.45) (xy -0.01 -0.45) (xy 1.27 -0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.63 0.63) (xy 0.76 0.63) (xy 0.76 -0.63) (xy 1.63 -0.63)
				)
				(width 0.2)
				(fill yes)
			)
		)
	)
	(pad "1" smd oval
		(at -13.9 -17 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd oval
		(at -13.9 -15 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd oval
		(at -13.9 -13 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" smd oval
		(at -13.9 -11 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd oval
		(at -13.9 -9 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd oval
		(at -13.9 -7 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "7" smd oval
		(at -13.9 -5 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd oval
		(at -13.9 -3 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd oval
		(at -13.9 -1 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd oval
		(at -13.9 1 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd oval
		(at -13.9 3 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" smd oval
		(at -13.9 5 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" smd oval
		(at -13.9 7 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" smd oval
		(at -13.9 9 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "15" smd oval
		(at -13.9 11 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" smd oval
		(at -13.9 13 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "17" smd oval
		(at -13.9 15 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" smd oval
		(at -13.9 17 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "19" smd oval
		(at -10 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" smd oval
		(at -8 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "21" smd oval
		(at -6 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" smd oval
		(at -4 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "23" smd oval
		(at -2 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" smd oval
		(at 0 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "25" smd oval
		(at 6 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" smd oval
		(at 8 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "27" smd oval
		(at 10 18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" smd oval
		(at 13.9 17 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "29" smd oval
		(at 13.9 15 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" smd oval
		(at 13.9 13 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "31" smd oval
		(at 13.9 11 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" smd oval
		(at 13.9 9 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" smd oval
		(at 13.9 7 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" smd oval
		(at 13.9 5 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" smd oval
		(at 13.9 3 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" smd oval
		(at 13.9 1 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" smd oval
		(at 13.9 -1 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" smd oval
		(at 13.9 -3 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" smd oval
		(at 13.9 -5 90)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" smd oval
		(at 13.9 -7 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" smd oval
		(at 13.9 -9 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" smd oval
		(at 13.9 -11 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" smd oval
		(at 13.9 -13 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" smd oval
		(at 13.9 -15 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" smd oval
		(at 13.9 -17 270)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" smd oval
		(at 10 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" smd oval
		(at 8 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" smd oval
		(at 6 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" smd oval
		(at -4 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" smd oval
		(at -6 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" smd oval
		(at -8 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" smd oval
		(at -10 -18.9)
		(size 0.9 1.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Carambola2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
