(footprint "RaspberryPi_Pico_Common_Unspecified"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry Pi Pico versatile common (Pico & Pico W) footprint for surface-mount or through-hole hand soldering, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
	(tags "module usb pcb antenna")
	(property "Reference" "REF**"
		(at 11.7475 24.765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RaspberryPi_Pico_Common_Unspecified"
		(at 0 27.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "Keep"
		(at 1 -5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep Out"
		(at 0 -36.195 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Out"
		(at 0 -20.6825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Copper"
		(at 1 -5.635 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Out"
		(at 1 -4.365 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "USB Cable"
		(at 0 -38.735 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep Out"
		(at 0 21.59 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed Copper Keep Out"
		(at 0 24.765 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "AGND Plane"
		(at 5.08 -7.62 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep"
		(at 0 -21.3175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Possible Antenna"
		(at 0 19.685 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed Copper Keep Out"
		(at -2.5 -14.25 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed Copper Keep Out"
		(at 3.1241 5.7 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed"
		(at 0 -24.6175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Copper"
		(at 0 -23.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.725 -24)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -2.425 -20.97)
		(size 1.85 1.85)
		(drill 1.85)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.425 -20.97)
		(size 1.85 1.85)
		(drill 1.85)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.725 -24)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Mask")
	)
	(pad "1" smd custom
		(at -9.69 -24.13)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at -8.89 -24.13)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at -9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "2" thru_hole circle
		(at -8.89 -21.59)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" smd custom
		(at -9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" thru_hole custom
		(at -8.89 -19.05)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd roundrect
		(at -9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "4" thru_hole circle
		(at -8.89 -16.51)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" smd roundrect
		(at -9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "5" thru_hole circle
		(at -8.89 -13.97)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd roundrect
		(at -9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "6" thru_hole circle
		(at -8.89 -11.43)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" smd roundrect
		(at -9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "7" thru_hole circle
		(at -8.89 -8.89)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" smd custom
		(at -9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "8" thru_hole custom
		(at -8.89 -6.35)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd roundrect
		(at -9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "9" thru_hole circle
		(at -8.89 -3.81)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" smd roundrect
		(at -9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "10" thru_hole circle
		(at -8.89 -1.27)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd roundrect
		(at -9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "11" thru_hole circle
		(at -8.89 1.27)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" smd roundrect
		(at -9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "12" thru_hole circle
		(at -8.89 3.81)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" smd custom
		(at -9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "13" thru_hole custom
		(at -8.89 6.35)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "14" smd roundrect
		(at -9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "14" thru_hole circle
		(at -8.89 8.89)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" smd roundrect
		(at -9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "15" thru_hole circle
		(at -8.89 11.43)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" smd roundrect
		(at -9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "16" thru_hole circle
		(at -8.89 13.97)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" smd roundrect
		(at -9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "17" thru_hole circle
		(at -8.89 16.51)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" smd custom
		(at -9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "18" thru_hole custom
		(at -8.89 19.05)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 0.6)
				(end 0.8 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.6 -0.6)
				(end 0.8 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "19" smd roundrect
		(at -9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "19" thru_hole circle
		(at -8.89 21.59)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" smd roundrect
		(at -9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "20" thru_hole circle
		(at -8.89 24.13)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 8.89 24.13)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" smd roundrect
		(at 9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "22" thru_hole circle
		(at 8.89 21.59)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" smd roundrect
		(at 9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "23" thru_hole custom
		(at 8.89 19.05)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 0.6)
				(end -0.4 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 -0.6)
				(end -0.4 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "23" smd custom
		(at 9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "24" thru_hole circle
		(at 8.89 16.51)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" smd roundrect
		(at 9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "25" thru_hole circle
		(at 8.89 13.97)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" smd roundrect
		(at 9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "26" thru_hole circle
		(at 8.89 11.43)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" smd roundrect
		(at 9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "27" thru_hole circle
		(at 8.89 8.89)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" smd roundrect
		(at 9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "28" thru_hole custom
		(at 8.89 6.35)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 0.6)
				(end -0.4 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 -0.6)
				(end -0.4 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "28" smd custom
		(at 9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "29" thru_hole circle
		(at 8.89 3.81)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" smd roundrect
		(at 9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "30" thru_hole circle
		(at 8.89 1.27)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" smd roundrect
		(at 9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "31" thru_hole circle
		(at 8.89 -1.27)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" smd roundrect
		(at 9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "32" thru_hole circle
		(at 8.89 -3.81)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" smd roundrect
		(at 9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "33" thru_hole custom
		(at 8.89 -6.35)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 0.6)
				(end -0.4 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 -0.6)
				(end -0.4 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "33" smd custom
		(at 9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "34" thru_hole circle
		(at 8.89 -8.89)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" smd roundrect
		(at 9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "35" thru_hole circle
		(at 8.89 -11.43)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" smd roundrect
		(at 9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "36" thru_hole circle
		(at 8.89 -13.97)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" smd roundrect
		(at 9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "37" thru_hole circle
		(at 8.89 -16.51)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" smd roundrect
		(at 9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "38" thru_hole custom
		(at 8.89 -19.05)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 0.6)
				(end -0.4 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 -0.6)
				(end -0.4 -0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "38" smd custom
		(at 9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "39" thru_hole circle
		(at 8.89 -21.59)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd roundrect
		(at 9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "40" thru_hole circle
		(at 8.89 -24.13)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" smd roundrect
		(at 9.69 -24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "F.Paste"
			"In6.Cu" "B.Paste" "In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu"
			"In13.Cu" "In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu"
			"In20.Cu" "In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu"
			"In27.Cu" "In28.Cu" "In29.Cu" "In30.Cu"
		)
		(name "Antenna Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.4 24.989895) (xy -7.1 21.339895) (xy -7.1 17) (xy 7.1 17) (xy 7.1 21.339895) (xy 2.4 24.989895)
				(xy 2.4 26) (xy -2.4 26)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D1-W")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.371222 4.800398) (xy -0.315502 4.744678) (xy -0.2427 4.714522) (xy -0.2033 4.7126) (xy 0.5841 4.7126)
				(xy 0.5841 6.6874) (xy -0.2033 6.6874) (xy -0.2427 6.685478) (xy -0.315502 6.655322) (xy -0.371222 6.599602)
				(xy -0.401378 6.5268) (xy -0.4033 6.4874) (xy -0.4033 4.9126) (xy -0.401378 4.8732)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D1-W")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1.3715 6.6874) (xy 0.5841 6.6874) (xy 0.5841 4.7126) (xy 1.3715 4.7126) (xy 1.4109 4.714522)
				(xy 1.483702 4.744677) (xy 1.539423 4.800398) (xy 1.569578 4.8732) (xy 1.5715 4.9126) (xy 1.5715 6.4874)
				(xy 1.569578 6.5268) (xy 1.539423 6.599602) (xy 1.483702 6.655323) (xy 1.4109 6.685478)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP6")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -3.015545 -10.052139) (xy -3.142167 -10.086068) (xy -3.255694 -10.151612) (xy -3.348388 -10.244306)
				(xy -3.413932 -10.357833) (xy -3.447861 -10.484455) (xy -3.45 -10.55) (xy -3.45 -14.25) (xy -1.55 -14.25)
				(xy -1.55 -10.55) (xy -1.552139 -10.484455) (xy -1.586068 -10.357833) (xy -1.651612 -10.244306)
				(xy -1.744306 -10.151612) (xy -1.857833 -10.086068) (xy -1.984455 -10.052139) (xy -2.05 -10.05)
				(xy -2.95 -10.05)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.947861 -24.815545) (xy -1.913932 -24.942167) (xy -1.848388 -25.055694) (xy -1.755694 -25.148388)
				(xy -1.642167 -25.213932) (xy -1.515545 -25.247861) (xy -1.45 -25.25) (xy -1 -25.25) (xy -1 -23.35)
				(xy -1.45 -23.35) (xy -1.515545 -23.352139) (xy -1.642167 -23.386068) (xy -1.755694 -23.451612)
				(xy -1.848388 -23.544306) (xy -1.913932 -23.657833) (xy -1.947861 -23.784455) (xy -1.95 -23.85)
				(xy -1.95 -24.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP4")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.55 -14.25) (xy -1.55 -17.95) (xy -1.552139 -18.015545) (xy -1.586067 -18.142167) (xy -1.651612 -18.255694)
				(xy -1.744306 -18.348388) (xy -1.857833 -18.413933) (xy -1.984455 -18.447861) (xy -2.05 -18.45)
				(xy -2.95 -18.45) (xy -3.015545 -18.447861) (xy -3.142167 -18.413933) (xy -3.255694 -18.348388)
				(xy -3.348388 -18.255694) (xy -3.413933 -18.142167) (xy -3.447861 -18.015545) (xy -3.45 -17.95)
				(xy -3.45 -14.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1 -23.35) (xy -0.55 -23.35) (xy -0.484455 -23.352139) (xy -0.357833 -23.386067) (xy -0.244306 -23.451612)
				(xy -0.151612 -23.544306) (xy -0.086067 -23.657833) (xy -0.052139 -23.784455) (xy -0.05 -23.85)
				(xy -0.05 -24.75) (xy -0.052139 -24.815545) (xy -0.086067 -24.942167) (xy -0.151612 -25.055694)
				(xy -0.244306 -25.148388) (xy -0.357833 -25.213933) (xy -0.484455 -25.247861) (xy -0.55 -25.25)
				(xy -1 -25.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.947861 -21.515545) (xy -0.913932 -21.642167) (xy -0.848388 -21.755694) (xy -0.755694 -21.848388)
				(xy -0.642167 -21.913932) (xy -0.515545 -21.947861) (xy -0.45 -21.95) (xy 0 -21.95) (xy 0 -20.05)
				(xy -0.45 -20.05) (xy -0.515545 -20.052139) (xy -0.642167 -20.086068) (xy -0.755694 -20.151612)
				(xy -0.848388 -20.244306) (xy -0.913932 -20.357833) (xy -0.947861 -20.484455) (xy -0.95 -20.55)
				(xy -0.95 -21.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.6 22.9) (xy 0 22.9)
				(arc
					(start 0 26.5)
					(mid -0.707107 26.207107)
					(end -1 25.5)
				)
				(xy -1 23.3) (xy -0.997807 23.236994) (xy -0.958867 23.117148) (xy -0.884799 23.015201) (xy -0.782852 22.941133)
				(xy -0.663006 22.902193)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 -20.05) (xy 0.45 -20.05) (xy 0.515545 -20.052139) (xy 0.642167 -20.086067) (xy 0.755694 -20.151612)
				(xy 0.848388 -20.244306) (xy 0.913933 -20.357833) (xy 0.947861 -20.484455) (xy 0.95 -20.55) (xy 0.95 -21.45)
				(xy 0.947861 -21.515545) (xy 0.913933 -21.642167) (xy 0.848388 -21.755694) (xy 0.755694 -21.848388)
				(xy 0.642167 -21.913933) (xy 0.515545 -21.947861) (xy 0.45 -21.95) (xy 0 -21.95)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.052139 -24.800545) (xy 0.086068 -24.927167) (xy 0.151612 -25.040694) (xy 0.244306 -25.133388)
				(xy 0.357833 -25.198932) (xy 0.484455 -25.232861) (xy 0.55 -25.235) (xy 1 -25.235) (xy 1 -23.335)
				(xy 0.55 -23.335) (xy 0.484455 -23.337139) (xy 0.357833 -23.371068) (xy 0.244306 -23.436612) (xy 0.151612 -23.529306)
				(xy 0.086068 -23.642833) (xy 0.052139 -23.769455) (xy 0.05 -23.835) (xy 0.05 -24.735)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP7")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.052139 -5.515545) (xy 0.086068 -5.642167) (xy 0.151612 -5.755694) (xy 0.244306 -5.848388)
				(xy 0.357833 -5.913932) (xy 0.484455 -5.947861) (xy 0.55 -5.95) (xy 1 -5.95) (xy 1 -4.05) (xy 0.55 -4.05)
				(xy 0.484455 -4.052139) (xy 0.357833 -4.086068) (xy 0.244306 -4.151612) (xy 0.151612 -4.244306)
				(xy 0.086068 -4.357833) (xy 0.052139 -4.484455) (xy 0.05 -4.55) (xy 0.05 -5.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.6 22.9) (xy 0.662964 22.902462) (xy 0.782728 22.941376) (xy 0.884606 23.015394) (xy 0.958624 23.117272)
				(xy 0.997538 23.237036) (xy 1 23.3)
				(arc
					(start 1 25.5)
					(mid 0.707107 26.207107)
					(end 0 26.5)
				)
				(xy 0 22.9)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1 -23.335) (xy 1.45 -23.335) (xy 1.515545 -23.337139) (xy 1.642167 -23.371067) (xy 1.755694 -23.436612)
				(xy 1.848388 -23.529306) (xy 1.913933 -23.642833) (xy 1.947861 -23.769455) (xy 1.95 -23.835) (xy 1.95 -24.735)
				(xy 1.947861 -24.800545) (xy 1.913933 -24.927167) (xy 1.848388 -25.040694) (xy 1.755694 -25.133388)
				(xy 1.642167 -25.198933) (xy 1.515545 -25.232861) (xy 1.45 -25.235) (xy 1 -25.235)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP7")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1 -4.05) (xy 1.45 -4.05) (xy 1.515545 -4.052139) (xy 1.642167 -4.086067) (xy 1.755694 -4.151612)
				(xy 1.848388 -4.244306) (xy 1.913933 -4.357833) (xy 1.947861 -4.484455) (xy 1.95 -4.55) (xy 1.95 -5.45)
				(xy 1.947861 -5.515545) (xy 1.913933 -5.642167) (xy 1.848388 -5.755694) (xy 1.755694 -5.848388)
				(xy 1.642167 -5.913933) (xy 1.515545 -5.947861) (xy 1.45 -5.95) (xy 1 -5.95)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start -3.54 25.5)
					(mid -3.247107 26.207107)
					(end -2.54 26.5)
				)
				(arc
					(start -2.54 22.9)
					(mid -3.247107 23.192893)
					(end -3.54 23.9)
				)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start -2.54 26.5)
					(mid -1.832893 26.207107)
					(end -1.54 25.5)
				)
				(arc
					(start -1.54 23.9)
					(mid -1.832893 23.192893)
					(end -2.54 22.9)
				)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 1.540141 25.499925)
					(mid 1.833034 26.207032)
					(end 2.540141 26.499925)
				)
				(arc
					(start 2.540141 22.899925)
					(mid 1.833034 23.192818)
					(end 1.540141 23.899925)
				)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 2.540141 26.499925)
					(mid 3.247248 26.207032)
					(end 3.540141 25.499925)
				)
				(arc
					(start 3.540141 23.899925)
					(mid 3.247248 23.192818)
					(end 2.540141 22.899925)
				)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D2-W")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 4.116278 5.7) (xy 4.097382 5.507285) (xy 4.041414 5.32191) (xy 3.950506 5.150937) (xy 3.82812 5.000877)
				(xy 3.678919 4.877447) (xy 3.508584 4.785348) (xy 3.323605 4.728087) (xy 3.131027 4.707846) (xy 2.938184 4.725396)
				(xy 2.752424 4.780069) (xy 2.58082 4.869781) (xy 2.429909 4.991116) (xy 2.305441 5.139452) (xy 2.212154 5.30914)
				(xy 2.153603 5.493715) (xy 2.132019 5.686147) (xy 2.148222 5.879107) (xy 2.201596 6.065245) (xy 2.290108 6.237471)
				(xy 2.410387 6.389225) (xy 2.557851 6.514726) (xy 2.726882 6.609195) (xy 2.911044 6.669033) (xy 3.103321 6.69196)
				(xy 3.29639 6.677105) (xy 3.482896 6.625031) (xy 3.655736 6.537724) (xy 3.808325 6.418507) (xy 3.934853 6.271923)
				(xy 4.0305 6.103555) (xy 4.091622 5.919816) (xy 4.115891 5.727703)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out D3-W")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 6.656278 5.7) (xy 6.637382 5.507285) (xy 6.581414 5.32191) (xy 6.490506 5.150937) (xy 6.36812 5.000877)
				(xy 6.218919 4.877447) (xy 6.048584 4.785348) (xy 5.863605 4.728087) (xy 5.671027 4.707846) (xy 5.478184 4.725396)
				(xy 5.292424 4.780069) (xy 5.12082 4.869781) (xy 4.969909 4.991116) (xy 4.845441 5.139452) (xy 4.752154 5.30914)
				(xy 4.693603 5.493715) (xy 4.672019 5.686147) (xy 4.688222 5.879107) (xy 4.741596 6.065245) (xy 4.830108 6.237471)
				(xy 4.950387 6.389225) (xy 5.097851 6.514726) (xy 5.266882 6.609195) (xy 5.451044 6.669033) (xy 5.643321 6.69196)
				(xy 5.83639 6.677105) (xy 6.022896 6.625031) (xy 6.195736 6.537724) (xy 6.348325 6.418507) (xy 6.474853 6.271923)
				(xy 6.5705 6.103555) (xy 6.631622 5.919816) (xy 6.655891 5.727703)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(name "Board Keep Out USB Cable")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -6.2 -47.65) (xy 6.2 -47.65) (xy 6.2 -27.25) (xy -6.2 -27.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.CrtYd")
		(name "USB Cable Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.75 -27.7) (xy -3.94 -27.7) (xy -3.94 -27.3) (xy 3.94 -27.3) (xy 3.94 -27.7) (xy 5.75 -27.7)
				(xy 5.75 -47.2) (xy -5.75 -47.2)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_DIP-40_W17.78mm_H8.51mm_Socket.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_Socketed.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H_Socketed.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_Socketed.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH_Socketed.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
