(footprint "RaspberryPi_Pico_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry Pi Pico (non-W) surface-mount footprint for reflow soldering with test points and debug pads, supports Raspberry Pi Pico 2 (non-W), https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
	(tags "module usb pcb swd")
	(property "Reference" "REF**"
		(at 11.7475 24.765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RaspberryPi_Pico_SMD"
		(at 0 27.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "AGND Plane"
		(at 5.08 -7.62 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Copper"
		(at 1 -5.635 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep"
		(at 1 -5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Out"
		(at 1 -4.365 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -2.725 -24)
		(size 1.1 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -2.54 23.9)
		(size 2.2 3.8)
		(drill
			(offset 0 0.8)
		)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -2.425 -20.97)
		(size 1.05 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 0 23.9)
		(size 2.2 3.8)
		(drill
			(offset 0 0.8)
		)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.425 -20.97)
		(size 1.05 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 2.54 23.9)
		(size 2.2 3.8)
		(drill
			(offset 0 0.8)
		)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at 2.725 -24)
		(size 1.1 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -9.69 -24.13)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "3" smd custom
		(at -9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd roundrect
		(at -9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "5" smd roundrect
		(at -9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "6" smd roundrect
		(at -9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "7" smd roundrect
		(at -9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "8" smd custom
		(at -9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd roundrect
		(at -9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "10" smd roundrect
		(at -9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "11" smd roundrect
		(at -9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "12" smd roundrect
		(at -9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "13" smd custom
		(at -9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "14" smd roundrect
		(at -9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "15" smd roundrect
		(at -9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "16" smd roundrect
		(at -9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "17" smd roundrect
		(at -9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "18" smd custom
		(at -9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "19" smd roundrect
		(at -9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "20" smd roundrect
		(at -9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "21" smd roundrect
		(at 9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "22" smd roundrect
		(at 9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "23" smd custom
		(at 9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "24" smd roundrect
		(at 9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "25" smd roundrect
		(at 9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "26" smd roundrect
		(at 9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "27" smd roundrect
		(at 9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "28" smd custom
		(at 9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "29" smd roundrect
		(at 9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "30" smd roundrect
		(at 9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "31" smd roundrect
		(at 9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "32" smd roundrect
		(at 9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "33" smd custom
		(at 9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "34" smd roundrect
		(at 9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "35" smd roundrect
		(at 9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "36" smd roundrect
		(at 9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "37" smd roundrect
		(at 9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "38" smd custom
		(at 9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "39" smd roundrect
		(at 9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "40" smd roundrect
		(at 9.69 -24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "D1" smd roundrect
		(at -2.54 23.9 90)
		(size 3.2 1.6)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "D2" smd custom
		(at 0 23.9 270)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 -0.6) (xy -0.8 0.6) (xy -0.6 0.8) (xy 1.6 0.8) (xy 1.6 -0.8) (xy -0.6 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 0.6)
				(end -0.4 0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.6 -0.6)
				(end -0.4 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.6 0)
				(end 2.4 0)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "D3" smd roundrect
		(at 2.54 23.9 90)
		(size 3.2 1.6)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "TP1" smd roundrect
		(at 0 -21)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP2" smd roundrect
		(at 1 -24.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP3" smd roundrect
		(at -1 -24.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP4" smd roundrect
		(at -2.5 -17.5)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP5" smd roundrect
		(at -2.5 -15)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP6" smd roundrect
		(at -2.5 -12.5)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP7")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.052139 -5.515545) (xy 0.086068 -5.642167) (xy 0.151612 -5.755694) (xy 0.244306 -5.848388)
				(xy 0.357833 -5.913932) (xy 0.484455 -5.947861) (xy 0.55 -5.95) (xy 1 -5.95) (xy 1 -4.05) (xy 0.55 -4.05)
				(xy 0.484455 -4.052139) (xy 0.357833 -4.086068) (xy 0.244306 -4.151612) (xy 0.151612 -4.244306)
				(xy 0.086068 -4.357833) (xy 0.052139 -4.484455) (xy 0.05 -4.55) (xy 0.05 -5.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP7")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1 -4.05) (xy 1.45 -4.05) (xy 1.515545 -4.052139) (xy 1.642167 -4.086067) (xy 1.755694 -4.151612)
				(xy 1.848388 -4.244306) (xy 1.913933 -4.357833) (xy 1.947861 -4.484455) (xy 1.95 -4.55) (xy 1.95 -5.45)
				(xy 1.947861 -5.515545) (xy 1.913933 -5.642167) (xy 1.848388 -5.755694) (xy 1.755694 -5.848388)
				(xy 1.642167 -5.913933) (xy 1.515545 -5.947861) (xy 1.45 -5.95) (xy 1 -5.95)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
