(footprint "RaspberryPi_Pico_W_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry Pi Pico W surface-mount footprint for reflow soldering with test points and debug pads (not compatible with non-wireless Pico), supports Raspberry Pi Pico 2 W, https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf")
	(tags "module usb pcb swd antenna")
	(property "Reference" "REF**"
		(at 11.7475 24.765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RaspberryPi_Pico_W_SMD"
		(at 0 27.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at -14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Antenna"
		(at 0 19.685 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep Out"
		(at 0 21.59 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 0 17.78 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep unobstructed by metal as far as possible in all dimensions"
		(at 0 33.9725 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2.4 GHz RF Keep Out"
		(at 0 31.75 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd oval
		(at -2.725 -24)
		(size 1.1 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd oval
		(at -2.425 -20.97)
		(size 1.05 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd oval
		(at 2.425 -20.97)
		(size 1.05 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd oval
		(at 2.725 -24)
		(size 1.1 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -9.69 -24.13)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "3" smd custom
		(at -9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd roundrect
		(at -9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "5" smd roundrect
		(at -9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "6" smd roundrect
		(at -9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "7" smd roundrect
		(at -9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "8" smd custom
		(at -9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd roundrect
		(at -9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "10" smd roundrect
		(at -9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "11" smd roundrect
		(at -9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "12" smd roundrect
		(at -9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "13" smd custom
		(at -9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "14" smd roundrect
		(at -9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "15" smd roundrect
		(at -9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "16" smd roundrect
		(at -9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "17" smd roundrect
		(at -9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "18" smd custom
		(at -9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "19" smd roundrect
		(at -9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "20" smd roundrect
		(at -9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "21" smd roundrect
		(at 9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "22" smd roundrect
		(at 9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "23" smd custom
		(at 9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "24" smd roundrect
		(at 9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "25" smd roundrect
		(at 9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "26" smd roundrect
		(at 9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "27" smd roundrect
		(at 9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "28" smd custom
		(at 9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "29" smd roundrect
		(at 9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "30" smd roundrect
		(at 9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "31" smd roundrect
		(at 9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "32" smd roundrect
		(at 9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "33" smd custom
		(at 9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "34" smd roundrect
		(at 9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "35" smd roundrect
		(at 9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "36" smd roundrect
		(at 9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "37" smd roundrect
		(at 9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "38" smd custom
		(at 9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "39" smd roundrect
		(at 9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "40" smd roundrect
		(at 9.69 -24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "D1" smd roundrect
		(at 0.5841 5.7)
		(size 1.5748 1.5748)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.127000254)
	)
	(pad "D2" smd circle
		(at 3.1241 5.7)
		(size 1.5748 1.5748)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at 5.6641 5.7)
		(size 1.5748 1.5748)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "TP1" smd roundrect
		(at 0 -21)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP2" smd roundrect
		(at 1 -24.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP3" smd roundrect
		(at -1 -24.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP4" smd roundrect
		(at -2.5 -16)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP5" smd roundrect
		(at -2.5 -13.5)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "TP6" smd roundrect
		(at -2.5 -11)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "F.Paste"
			"In6.Cu" "B.Paste" "In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu"
			"In13.Cu" "In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu"
			"In20.Cu" "In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu"
			"In27.Cu" "In28.Cu" "In29.Cu" "In30.Cu"
		)
		(name "RF Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -21 25) (xy 21 25) (xy 21 35) (xy -21 35)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "F.Paste"
			"In6.Cu" "B.Paste" "In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu"
			"In13.Cu" "In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu"
			"In20.Cu" "In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu"
			"In27.Cu" "In28.Cu" "In29.Cu" "In30.Cu"
		)
		(name "Antenna Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.4 24.989895) (xy -7.1 21.339895) (xy -7.1 17) (xy 7.1 17) (xy 7.1 21.339895) (xy 2.4 24.989895)
				(xy 2.4 25) (xy -2.4 25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(name "Board Keep Out Suggestion RF")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 7.1 26) (xy 21 26) (xy 21 35) (xy -21 35) (xy -21 26) (xy -7.1 26) (xy -7.1 17) (xy 7.1 17)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
