(footprint "RaspberryPi_Pico_W_SMD_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry Pi Pico W surface-mount footprint with debug pads for hand soldering (not compatible with non-wireless Pico), supports Raspberry Pi Pico 2 W, https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf")
	(tags "module usb pcb swd antenna")
	(property "Reference" "REF**"
		(at 11.7475 24.765 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RaspberryPi_Pico_W_SMD_HandSolder"
		(at 0 27.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Antenna"
		(at 0 19.685 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at -14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep unobstructed by metal as far as possible in all dimensions"
		(at 0 33.9725 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "USB Cable"
		(at 0 -38.735 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep Out"
		(at 0 -36.195 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed"
		(at 0 -24.6175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Out"
		(at 0 -20.6825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 14.05 26.67 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "^ Suggested board edge for RF ^"
		(at 0 17.78 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep Out"
		(at 0 21.59 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2.4 GHz RF Keep Out"
		(at 0 31.75 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Copper"
		(at 0 -23.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Exposed Copper Keep Out"
		(at -2.5 -14.25 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Keep"
		(at 0 -21.3175 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset -0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" np_thru_hole circle
		(at -2.725 -24)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -2.425 -20.97)
		(size 1.85 1.85)
		(drill 1.85)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.425 -20.97)
		(size 1.85 1.85)
		(drill 1.85)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.725 -24)
		(size 2.2 2.2)
		(drill 2.2)
		(layers "*.Mask")
	)
	(pad "" smd rect
		(at 8.89 -24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 -1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 1.27)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 3.81)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 6.35)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 8.89)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 11.43)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 13.97)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 16.51)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 19.05)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 21.59)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 8.89 24.13)
		(size 3.8 2.2)
		(drill
			(offset 0.8 0)
		)
		(layers "F.Paste")
	)
	(pad "1" smd custom
		(at -9.69 -24.13)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "3" smd custom
		(at -9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd roundrect
		(at -9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "5" smd roundrect
		(at -9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "6" smd roundrect
		(at -9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "7" smd roundrect
		(at -9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "8" smd custom
		(at -9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "9" smd roundrect
		(at -9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "10" smd roundrect
		(at -9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "11" smd roundrect
		(at -9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "12" smd roundrect
		(at -9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "13" smd custom
		(at -9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "14" smd roundrect
		(at -9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "15" smd roundrect
		(at -9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "16" smd roundrect
		(at -9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "17" smd roundrect
		(at -9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "18" smd custom
		(at -9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.8 0)
				(end 0 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.6 -0.6) (xy 1.6 0.6) (xy 1.4 0.8) (xy -0.8 0.8) (xy -0.8 -0.8) (xy 1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 -0.6)
				(end 1.6 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 1.4 0.6)
				(end 1.6 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "19" smd roundrect
		(at -9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "20" smd roundrect
		(at -9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "21" smd roundrect
		(at 9.69 24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "22" smd roundrect
		(at 9.69 21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "23" smd custom
		(at 9.69 19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "24" smd roundrect
		(at 9.69 16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "25" smd roundrect
		(at 9.69 13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "26" smd roundrect
		(at 9.69 11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "27" smd roundrect
		(at 9.69 8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "28" smd custom
		(at 9.69 6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "29" smd roundrect
		(at 9.69 3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "30" smd roundrect
		(at 9.69 1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "31" smd roundrect
		(at 9.69 -1.27)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "32" smd roundrect
		(at 9.69 -3.81)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "33" smd custom
		(at 9.69 -6.35)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "34" smd roundrect
		(at 9.69 -8.89)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "35" smd roundrect
		(at 9.69 -11.43)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "36" smd roundrect
		(at 9.69 -13.97)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "37" smd roundrect
		(at 9.69 -16.51)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "38" smd custom
		(at 9.69 -19.05)
		(size 1.6 0.8)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0.8 0)
				(end 1.6 0)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.6 -0.6) (xy -1.6 0.6) (xy -1.4 0.8) (xy 0.8 0.8) (xy 0.8 -0.8) (xy -1.4 -0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 -0.6)
				(end -1.2 -0.6)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -1.4 0.6)
				(end -1.2 0.6)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "39" smd roundrect
		(at 9.69 -21.59)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "40" smd roundrect
		(at 9.69 -24.13)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
	)
	(pad "D1" thru_hole roundrect
		(at 0.5841 5.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.125)
	)
	(pad "D2" thru_hole circle
		(at 3.1241 5.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D3" thru_hole circle
		(at 5.6641 5.7)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "F.Paste"
			"In6.Cu" "B.Paste" "In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu"
			"In13.Cu" "In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu"
			"In20.Cu" "In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu"
			"In27.Cu" "In28.Cu" "In29.Cu" "In30.Cu"
		)
		(name "RF Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -21 25) (xy 21 25) (xy 21 35) (xy -21 35)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "F.Paste"
			"In6.Cu" "B.Paste" "In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu"
			"In13.Cu" "In14.Cu" "In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu"
			"In20.Cu" "In21.Cu" "In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu"
			"In27.Cu" "In28.Cu" "In29.Cu" "In30.Cu"
		)
		(name "Antenna Copper Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.4 24.989895) (xy -7.1 21.339895) (xy -7.1 17) (xy 7.1 17) (xy 7.1 21.339895) (xy 2.4 24.989895)
				(xy 2.4 25) (xy -2.4 25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP6")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -3.015545 -10.052139) (xy -3.142167 -10.086068) (xy -3.255694 -10.151612) (xy -3.348388 -10.244306)
				(xy -3.413932 -10.357833) (xy -3.447861 -10.484455) (xy -3.45 -10.55) (xy -3.45 -14.25) (xy -1.55 -14.25)
				(xy -1.55 -10.55) (xy -1.552139 -10.484455) (xy -1.586068 -10.357833) (xy -1.651612 -10.244306)
				(xy -1.744306 -10.151612) (xy -1.857833 -10.086068) (xy -1.984455 -10.052139) (xy -2.05 -10.05)
				(xy -2.95 -10.05)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.947861 -24.815545) (xy -1.913932 -24.942167) (xy -1.848388 -25.055694) (xy -1.755694 -25.148388)
				(xy -1.642167 -25.213932) (xy -1.515545 -25.247861) (xy -1.45 -25.25) (xy -1 -25.25) (xy -1 -23.35)
				(xy -1.45 -23.35) (xy -1.515545 -23.352139) (xy -1.642167 -23.386068) (xy -1.755694 -23.451612)
				(xy -1.848388 -23.544306) (xy -1.913932 -23.657833) (xy -1.947861 -23.784455) (xy -1.95 -23.85)
				(xy -1.95 -24.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP4")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.55 -14.25) (xy -1.55 -17.95) (xy -1.552139 -18.015545) (xy -1.586067 -18.142167) (xy -1.651612 -18.255694)
				(xy -1.744306 -18.348388) (xy -1.857833 -18.413933) (xy -1.984455 -18.447861) (xy -2.05 -18.45)
				(xy -2.95 -18.45) (xy -3.015545 -18.447861) (xy -3.142167 -18.413933) (xy -3.255694 -18.348388)
				(xy -3.348388 -18.255694) (xy -3.413933 -18.142167) (xy -3.447861 -18.015545) (xy -3.45 -17.95)
				(xy -3.45 -14.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP3")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1 -23.35) (xy -0.55 -23.35) (xy -0.484455 -23.352139) (xy -0.357833 -23.386067) (xy -0.244306 -23.451612)
				(xy -0.151612 -23.544306) (xy -0.086067 -23.657833) (xy -0.052139 -23.784455) (xy -0.05 -23.85)
				(xy -0.05 -24.75) (xy -0.052139 -24.815545) (xy -0.086067 -24.942167) (xy -0.151612 -25.055694)
				(xy -0.244306 -25.148388) (xy -0.357833 -25.213933) (xy -0.484455 -25.247861) (xy -0.55 -25.25)
				(xy -1 -25.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.947861 -21.515545) (xy -0.913932 -21.642167) (xy -0.848388 -21.755694) (xy -0.755694 -21.848388)
				(xy -0.642167 -21.913932) (xy -0.515545 -21.947861) (xy -0.45 -21.95) (xy 0 -21.95) (xy 0 -20.05)
				(xy -0.45 -20.05) (xy -0.515545 -20.052139) (xy -0.642167 -20.086068) (xy -0.755694 -20.151612)
				(xy -0.848388 -20.244306) (xy -0.913932 -20.357833) (xy -0.947861 -20.484455) (xy -0.95 -20.55)
				(xy -0.95 -21.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP1")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 -20.05) (xy 0.45 -20.05) (xy 0.515545 -20.052139) (xy 0.642167 -20.086067) (xy 0.755694 -20.151612)
				(xy 0.848388 -20.244306) (xy 0.913933 -20.357833) (xy 0.947861 -20.484455) (xy 0.95 -20.55) (xy 0.95 -21.45)
				(xy 0.947861 -21.515545) (xy 0.913933 -21.642167) (xy 0.848388 -21.755694) (xy 0.755694 -21.848388)
				(xy 0.642167 -21.913933) (xy 0.515545 -21.947861) (xy 0.45 -21.95) (xy 0 -21.95)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.052139 -24.800545) (xy 0.086068 -24.927167) (xy 0.151612 -25.040694) (xy 0.244306 -25.133388)
				(xy 0.357833 -25.198932) (xy 0.484455 -25.232861) (xy 0.55 -25.235) (xy 1 -25.235) (xy 1 -23.335)
				(xy 0.55 -23.335) (xy 0.484455 -23.337139) (xy 0.357833 -23.371068) (xy 0.244306 -23.436612) (xy 0.151612 -23.529306)
				(xy 0.086068 -23.642833) (xy 0.052139 -23.769455) (xy 0.05 -23.835) (xy 0.05 -24.735)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Paste")
		(name "Pad Keep Out TP2")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 1 -23.335) (xy 1.45 -23.335) (xy 1.515545 -23.337139) (xy 1.642167 -23.371067) (xy 1.755694 -23.436612)
				(xy 1.848388 -23.529306) (xy 1.913933 -23.642833) (xy 1.947861 -23.769455) (xy 1.95 -23.835) (xy 1.95 -24.735)
				(xy 1.947861 -24.800545) (xy 1.913933 -24.927167) (xy 1.848388 -25.040694) (xy 1.755694 -25.133388)
				(xy 1.642167 -25.198933) (xy 1.515545 -25.232861) (xy 1.45 -25.235) (xy 1 -25.235)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(name "Board Keep Out USB Cable")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -6.2 -47.65) (xy 6.2 -47.65) (xy 6.2 -27.25) (xy -6.2 -27.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(name "Board Keep Out Suggestion RF")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 7.1 26) (xy 21 26) (xy 21 35) (xy -21 35) (xy -21 26) (xy -7.1 26) (xy -7.1 17) (xy 7.1 17)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.CrtYd")
		(name "USB Cable Keep Out")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -5.75 -27.7) (xy -3.94 -27.7) (xy -3.94 -27.3) (xy 3.94 -27.3) (xy 3.94 -27.7) (xy 5.75 -27.7)
				(xy 5.75 -47.2) (xy -5.75 -47.2)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
