(footprint "Vybronics_VZ30C1T8219732L"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Vibration motor, 2.3-3.2V, 14000rpm, 0.7G, https://www.vybronics.com/wp-content/uploads/datasheet-files/Vybronics-VZ30C1T8219732L-datasheet.pdf")
	(tags "vibration motor Vybronics")
	(property "Reference" "REF**"
		(at 0 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vybronics_VZ30C1T8219732L"
		(at 0 6.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.85 -2.315 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.85 -0.905 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.85 0.505 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 -2.315 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 -0.905 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.85 0.505 270)
		(size 1.07 1.4)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.65 -4.35 270)
		(size 1.3 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.65 -4.35 270)
		(size 1.3 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -0.8 1.525)
		(size 1 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0 -3.85 270)
		(size 1.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0 -0.95 270)
		(size 4.3 3.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "SH" smd rect
		(at 0.8 1.525)
		(size 1 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Motors.3dshapes/Vybronics_VZ30C1T8219732L.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
