(footprint "Mounting_Wuerth_WA-SMSI-M1.6_H2mm_9774020633"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole M1.6, height 2, Wuerth electronics 9774020633 (https://katalog.we-online.com/em/datasheet/9774020633.pdf), generated with kicad-footprint-generator")
	(tags "Mounting M1.6 9774020633")
	(property "Reference" "REF**"
		(at 0 -2.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSI-M1.6_H2mm_9774020633"
		(at 0 2.95 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.06066 -1.06066)
		(size 0.4 0.4)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.101235 0.76066)
				(mid 0.212132 0.212132)
				(end 0.76066 -0.101235)
				(width 0.2)
			)
			(gr_arc
				(start -0.204251 0.76066)
				(mid 0.141421 0.141421)
				(end 0.76066 -0.204251)
				(width 0.2)
			)
			(gr_arc
				(start -0.306819 0.76066)
				(mid 0.070711 0.070711)
				(end 0.76066 -0.306819)
				(width 0.2)
			)
			(gr_arc
				(start -0.409034 0.76066)
				(mid 0 0)
				(end 0.76066 -0.409034)
				(width 0.2)
			)
			(gr_arc
				(start -0.510963 0.76066)
				(mid -0.070711 -0.070711)
				(end 0.76066 -0.510963)
				(width 0.2)
			)
			(gr_arc
				(start -0.61266 0.76066)
				(mid -0.141421 -0.141421)
				(end 0.76066 -0.61266)
				(width 0.2)
			)
			(gr_arc
				(start -0.714164 0.76066)
				(mid -0.212132 -0.212132)
				(end 0.76066 -0.714164)
				(width 0.2)
			)
			(gr_line
				(start 0.76066 -0.101235)
				(end 0.76066 -0.714164)
				(width 0.2)
			)
			(gr_line
				(start -0.101235 0.76066)
				(end -0.714164 0.76066)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -1.06066 1.06066)
		(size 0.4 0.4)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.76066 0.101235)
				(mid 0.212132 -0.212132)
				(end -0.101235 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.204251)
				(mid 0.141421 -0.141421)
				(end -0.204251 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.306819)
				(mid 0.070711 -0.070711)
				(end -0.306819 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.409034)
				(mid 0 0)
				(end -0.409034 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.510963)
				(mid -0.070711 0.070711)
				(end -0.510963 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.61266)
				(mid -0.141421 0.141421)
				(end -0.61266 -0.76066)
				(width 0.2)
			)
			(gr_arc
				(start 0.76066 0.714164)
				(mid -0.212132 0.212132)
				(end -0.714164 -0.76066)
				(width 0.2)
			)
			(gr_line
				(start -0.101235 -0.76066)
				(end -0.714164 -0.76066)
				(width 0.2)
			)
			(gr_line
				(start 0.76066 0.101235)
				(end 0.76066 0.714164)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 2.1 2.1)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 1.06066 -1.06066)
		(size 0.4 0.4)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.76066 -0.101235)
				(mid -0.212132 0.212132)
				(end 0.101235 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.204251)
				(mid -0.141421 0.141421)
				(end 0.204251 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.306819)
				(mid -0.070711 0.070711)
				(end 0.306819 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.409034)
				(mid 0 0)
				(end 0.409034 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.510963)
				(mid 0.070711 -0.070711)
				(end 0.510963 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.61266)
				(mid 0.141421 -0.141421)
				(end 0.61266 0.76066)
				(width 0.2)
			)
			(gr_arc
				(start -0.76066 -0.714164)
				(mid 0.212132 -0.212132)
				(end 0.714164 0.76066)
				(width 0.2)
			)
			(gr_line
				(start 0.101235 0.76066)
				(end 0.714164 0.76066)
				(width 0.2)
			)
			(gr_line
				(start -0.76066 -0.101235)
				(end -0.76066 -0.714164)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.06066 1.06066)
		(size 0.4 0.4)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.101235 -0.76066)
				(mid -0.212132 -0.212132)
				(end -0.76066 0.101235)
				(width 0.2)
			)
			(gr_arc
				(start 0.204251 -0.76066)
				(mid -0.141421 -0.141421)
				(end -0.76066 0.204251)
				(width 0.2)
			)
			(gr_arc
				(start 0.306819 -0.76066)
				(mid -0.070711 -0.070711)
				(end -0.76066 0.306819)
				(width 0.2)
			)
			(gr_arc
				(start 0.409034 -0.76066)
				(mid 0 0)
				(end -0.76066 0.409034)
				(width 0.2)
			)
			(gr_arc
				(start 0.510963 -0.76066)
				(mid 0.070711 0.070711)
				(end -0.76066 0.510963)
				(width 0.2)
			)
			(gr_arc
				(start 0.61266 -0.76066)
				(mid 0.141421 0.141421)
				(end -0.76066 0.61266)
				(width 0.2)
			)
			(gr_arc
				(start 0.714164 -0.76066)
				(mid 0.212132 0.212132)
				(end -0.76066 0.714164)
				(width 0.2)
			)
			(gr_line
				(start -0.76066 0.101235)
				(end -0.76066 0.714164)
				(width 0.2)
			)
			(gr_line
				(start 0.101235 -0.76066)
				(end 0.714164 -0.76066)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -1.525 0)
		(size 0.442 0.442)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -1.525)
		(size 0.442 0.442)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 1.525)
		(size 0.442 0.442)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 1.525 0)
		(size 0.95 0.95)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -1.525 0)
				(end 0 0)
				(width 0.95)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSI-M1.6_H2mm_9774020633.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
