(footprint "Mounting_Wuerth_WA-SMSI-M1.6_H6mm_ThreadDepth2mm_97730606332"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside blind hole M1.6, height 6, Wuerth electronics 97730606332 (https://katalog.we-online.com/em/datasheet/97730606332.pdf), generated with kicad-footprint-generator")
	(tags "Mounting M1.6 97730606332")
	(property "Reference" "REF**"
		(at 0 -2.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSI-M1.6_H6mm_ThreadDepth2mm_97730606332"
		(at 0 2.95 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at 0 -1.25)
		(size 0.65 0.65)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.259808 0.6)
				(mid 0.392514 0.670403)
				(end 0.7 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -0.466369 0.6)
				(mid 0.365311 0.538278)
				(end 0.8 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -0.622495 0.6)
				(mid 0.35338 0.422279)
				(end 0.9 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -0.759934 0.6)
				(mid 0.346458 0.311934)
				(end 1 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -0.887412 0.6)
				(mid 0.341941 0.204497)
				(end 1.1 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.008712 0.6)
				(mid 0.338781 0.098815)
				(end 1.2 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.125833 0.6)
				(mid 0.336465 -0.005704)
				(end 1.3 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.23996 0.6)
				(mid 0.334706 -0.109401)
				(end 1.4 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.351851 0.6)
				(mid 0.333335 -0.212494)
				(end 1.5 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.462019 0.6)
				(mid 0.332242 -0.315125)
				(end 1.6 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.570828 0.6)
				(mid 0.331355 -0.417394)
				(end 1.7 1.25)
				(width 0.2)
			)
			(gr_arc
				(start -1.678541 0.6)
				(mid 0.330625 -0.519375)
				(end 1.8 1.25)
				(width 0.2)
			)
			(gr_line
				(start 0.7 1.25)
				(end 1.8 1.25)
				(width 0.2)
			)
			(gr_line
				(start -0.259808 0.6)
				(end -1.678541 0.6)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 0 1.25)
		(size 0.65 0.65)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.259808 -0.6)
				(mid -0.392514 -0.670403)
				(end -0.7 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 0.466369 -0.6)
				(mid -0.365311 -0.538278)
				(end -0.8 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 0.622495 -0.6)
				(mid -0.35338 -0.422279)
				(end -0.9 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 0.759934 -0.6)
				(mid -0.346458 -0.311934)
				(end -1 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 0.887412 -0.6)
				(mid -0.341941 -0.204497)
				(end -1.1 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.008712 -0.6)
				(mid -0.338781 -0.098815)
				(end -1.2 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.125833 -0.6)
				(mid -0.336465 0.005704)
				(end -1.3 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.23996 -0.6)
				(mid -0.334706 0.109401)
				(end -1.4 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.351851 -0.6)
				(mid -0.333335 0.212494)
				(end -1.5 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.462019 -0.6)
				(mid -0.332242 0.315125)
				(end -1.6 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.570828 -0.6)
				(mid -0.331355 0.417394)
				(end -1.7 -1.25)
				(width 0.2)
			)
			(gr_arc
				(start 1.678541 -0.6)
				(mid -0.330625 0.519375)
				(end -1.8 -1.25)
				(width 0.2)
			)
			(gr_line
				(start -0.7 -1.25)
				(end -1.8 -1.25)
				(width 0.2)
			)
			(gr_line
				(start 0.259808 -0.6)
				(end 1.678541 -0.6)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -1.25 0)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -1.25)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 1.25)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 1.25 0)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -1.25 0)
				(end 0 0)
				(width 1.5)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSI-M1.6_H6mm_ThreadDepth2mm_97730606332.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
