(footprint "Mounting_Wuerth_WA-SMSR-M3_H2.6mm_ReverseMount_9775026360"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole M3, height 2.6, Wuerth electronics 9775026360 (https://katalog.we-online.com/em/datasheet/9775026360.pdf), generated with kicad-footprint-generator")
	(tags "Mounting M3 9775026360")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSR-M3_H2.6mm_ReverseMount_9775026360"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.094804 -2.094804)
		(size 0.6725 0.6725)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.24231 1.594804)
				(mid 0.404819 0.404819)
				(end 1.594804 -0.24231)
				(width 0.2)
			)
			(gr_arc
				(start -0.3398 1.594804)
				(mid 0.337349 0.337349)
				(end 1.594804 -0.3398)
				(width 0.2)
			)
			(gr_arc
				(start -0.437132 1.594804)
				(mid 0.269879 0.269879)
				(end 1.594804 -0.437132)
				(width 0.2)
			)
			(gr_arc
				(start -0.534324 1.594804)
				(mid 0.202409 0.202409)
				(end 1.594804 -0.534324)
				(width 0.2)
			)
			(gr_arc
				(start -0.631391 1.594804)
				(mid 0.13494 0.13494)
				(end 1.594804 -0.631391)
				(width 0.2)
			)
			(gr_arc
				(start -0.728345 1.594804)
				(mid 0.06747 0.06747)
				(end 1.594804 -0.728345)
				(width 0.2)
			)
			(gr_arc
				(start -0.825197 1.594804)
				(mid 0 0)
				(end 1.594804 -0.825197)
				(width 0.2)
			)
			(gr_arc
				(start -0.921958 1.594804)
				(mid -0.06747 -0.06747)
				(end 1.594804 -0.921958)
				(width 0.2)
			)
			(gr_arc
				(start -1.018637 1.594804)
				(mid -0.13494 -0.13494)
				(end 1.594804 -1.018637)
				(width 0.2)
			)
			(gr_arc
				(start -1.115239 1.594804)
				(mid -0.202409 -0.202409)
				(end 1.594804 -1.115239)
				(width 0.2)
			)
			(gr_arc
				(start -1.211773 1.594804)
				(mid -0.269879 -0.269879)
				(end 1.594804 -1.211773)
				(width 0.2)
			)
			(gr_arc
				(start -1.308244 1.594804)
				(mid -0.337349 -0.337349)
				(end 1.594804 -1.308244)
				(width 0.2)
			)
			(gr_arc
				(start -1.404657 1.594804)
				(mid -0.404819 -0.404819)
				(end 1.594804 -1.404657)
				(width 0.2)
			)
			(gr_arc
				(start -1.404657 1.594804)
				(mid -0.404819 -0.404819)
				(end 1.594804 -1.404657)
				(width 0.2)
			)
			(gr_line
				(start 1.594804 -0.24231)
				(end 1.594804 -1.404657)
				(width 0.2)
			)
			(gr_line
				(start -0.24231 1.594804)
				(end -1.404657 1.594804)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.094804 2.094804)
		(size 0.6725 0.6725)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.594804 0.24231)
				(mid 0.404819 -0.404819)
				(end -0.24231 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.3398)
				(mid 0.337349 -0.337349)
				(end -0.3398 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.437132)
				(mid 0.269879 -0.269879)
				(end -0.437132 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.534324)
				(mid 0.202409 -0.202409)
				(end -0.534324 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.631391)
				(mid 0.13494 -0.13494)
				(end -0.631391 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.728345)
				(mid 0.06747 -0.06747)
				(end -0.728345 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.825197)
				(mid 0 0)
				(end -0.825197 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 0.921958)
				(mid -0.06747 0.06747)
				(end -0.921958 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.018637)
				(mid -0.13494 0.13494)
				(end -1.018637 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.115239)
				(mid -0.202409 0.202409)
				(end -1.115239 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.211773)
				(mid -0.269879 0.269879)
				(end -1.211773 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.308244)
				(mid -0.337349 0.337349)
				(end -1.308244 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.404657)
				(mid -0.404819 0.404819)
				(end -1.404657 -1.594804)
				(width 0.2)
			)
			(gr_arc
				(start 1.594804 1.404657)
				(mid -0.404819 0.404819)
				(end -1.404657 -1.594804)
				(width 0.2)
			)
			(gr_line
				(start -0.24231 -1.594804)
				(end -1.404657 -1.594804)
				(width 0.2)
			)
			(gr_line
				(start 1.594804 0.24231)
				(end 1.594804 1.404657)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 4.4 4.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 2.094804 -2.094804)
		(size 0.6725 0.6725)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.594804 -0.24231)
				(mid -0.404819 0.404819)
				(end 0.24231 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.3398)
				(mid -0.337349 0.337349)
				(end 0.3398 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.437132)
				(mid -0.269879 0.269879)
				(end 0.437132 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.534324)
				(mid -0.202409 0.202409)
				(end 0.534324 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.631391)
				(mid -0.13494 0.13494)
				(end 0.631391 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.728345)
				(mid -0.06747 0.06747)
				(end 0.728345 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.825197)
				(mid 0 0)
				(end 0.825197 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -0.921958)
				(mid 0.06747 -0.06747)
				(end 0.921958 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.018637)
				(mid 0.13494 -0.13494)
				(end 1.018637 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.115239)
				(mid 0.202409 -0.202409)
				(end 1.115239 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.211773)
				(mid 0.269879 -0.269879)
				(end 1.211773 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.308244)
				(mid 0.337349 -0.337349)
				(end 1.308244 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.404657)
				(mid 0.404819 -0.404819)
				(end 1.404657 1.594804)
				(width 0.2)
			)
			(gr_arc
				(start -1.594804 -1.404657)
				(mid 0.404819 -0.404819)
				(end 1.404657 1.594804)
				(width 0.2)
			)
			(gr_line
				(start 0.24231 1.594804)
				(end 1.404657 1.594804)
				(width 0.2)
			)
			(gr_line
				(start -1.594804 -0.24231)
				(end -1.594804 -1.404657)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.094804 2.094804)
		(size 0.6725 0.6725)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.24231 -1.594804)
				(mid -0.404819 -0.404819)
				(end -1.594804 0.24231)
				(width 0.2)
			)
			(gr_arc
				(start 0.3398 -1.594804)
				(mid -0.337349 -0.337349)
				(end -1.594804 0.3398)
				(width 0.2)
			)
			(gr_arc
				(start 0.437132 -1.594804)
				(mid -0.269879 -0.269879)
				(end -1.594804 0.437132)
				(width 0.2)
			)
			(gr_arc
				(start 0.534324 -1.594804)
				(mid -0.202409 -0.202409)
				(end -1.594804 0.534324)
				(width 0.2)
			)
			(gr_arc
				(start 0.631391 -1.594804)
				(mid -0.13494 -0.13494)
				(end -1.594804 0.631391)
				(width 0.2)
			)
			(gr_arc
				(start 0.728345 -1.594804)
				(mid -0.06747 -0.06747)
				(end -1.594804 0.728345)
				(width 0.2)
			)
			(gr_arc
				(start 0.825197 -1.594804)
				(mid 0 0)
				(end -1.594804 0.825197)
				(width 0.2)
			)
			(gr_arc
				(start 0.921958 -1.594804)
				(mid 0.06747 0.06747)
				(end -1.594804 0.921958)
				(width 0.2)
			)
			(gr_arc
				(start 1.018637 -1.594804)
				(mid 0.13494 0.13494)
				(end -1.594804 1.018637)
				(width 0.2)
			)
			(gr_arc
				(start 1.115239 -1.594804)
				(mid 0.202409 0.202409)
				(end -1.594804 1.115239)
				(width 0.2)
			)
			(gr_arc
				(start 1.211773 -1.594804)
				(mid 0.269879 0.269879)
				(end -1.594804 1.211773)
				(width 0.2)
			)
			(gr_arc
				(start 1.308244 -1.594804)
				(mid 0.337349 0.337349)
				(end -1.594804 1.308244)
				(width 0.2)
			)
			(gr_arc
				(start 1.404657 -1.594804)
				(mid 0.404819 0.404819)
				(end -1.594804 1.404657)
				(width 0.2)
			)
			(gr_arc
				(start 1.404657 -1.594804)
				(mid 0.404819 0.404819)
				(end -1.594804 1.404657)
				(width 0.2)
			)
			(gr_line
				(start -1.594804 0.24231)
				(end -1.594804 1.404657)
				(width 0.2)
			)
			(gr_line
				(start 0.24231 -1.594804)
				(end 1.404657 -1.594804)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.975 0)
		(size 0.942 0.942)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.975)
		(size 0.942 0.942)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.975)
		(size 0.942 0.942)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.975 0)
		(size 1.45 1.45)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.975 0)
				(end 0 0)
				(width 1.45)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSR-M3_H2.6mm_ReverseMount_9775026360.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
