(footprint "Mounting_Wuerth_WA-SMSSR-3.3mm_H10mm_SnapRivet_9776100960"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole 3.3mm, height 10, Wuerth electronics 9776100960 (https://katalog.we-online.com/em/datasheet/9776100960R.pdf), generated with kicad-footprint-generator")
	(tags "Mounting 3.3mm 9776100960")
	(property "Reference" "REF**"
		(at 0 -4.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMSSR-3.3mm_H10mm_SnapRivet_9776100960"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -2.077126 -2.077126)
		(size 0.6975 0.6975)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.208831 1.577126)
				(mid 0.422496 0.422496)
				(end 1.577126 -0.208831)
				(width 0.2)
			)
			(gr_arc
				(start -0.310669 1.577126)
				(mid 0.35208 0.35208)
				(end 1.577126 -0.310669)
				(width 0.2)
			)
			(gr_arc
				(start -0.412325 1.577126)
				(mid 0.281664 0.281664)
				(end 1.577126 -0.412325)
				(width 0.2)
			)
			(gr_arc
				(start -0.51382 1.577126)
				(mid 0.211248 0.211248)
				(end 1.577126 -0.51382)
				(width 0.2)
			)
			(gr_arc
				(start -0.615172 1.577126)
				(mid 0.140832 0.140832)
				(end 1.577126 -0.615172)
				(width 0.2)
			)
			(gr_arc
				(start -0.716397 1.577126)
				(mid 0.070416 0.070416)
				(end 1.577126 -0.716397)
				(width 0.2)
			)
			(gr_arc
				(start -0.817508 1.577126)
				(mid 0 0)
				(end 1.577126 -0.817508)
				(width 0.2)
			)
			(gr_arc
				(start -0.918517 1.577126)
				(mid -0.070416 -0.070416)
				(end 1.577126 -0.918517)
				(width 0.2)
			)
			(gr_arc
				(start -1.019433 1.577126)
				(mid -0.140832 -0.140832)
				(end 1.577126 -1.019433)
				(width 0.2)
			)
			(gr_arc
				(start -1.120266 1.577126)
				(mid -0.211248 -0.211248)
				(end 1.577126 -1.120266)
				(width 0.2)
			)
			(gr_arc
				(start -1.221022 1.577126)
				(mid -0.281664 -0.281664)
				(end 1.577126 -1.221022)
				(width 0.2)
			)
			(gr_arc
				(start -1.32171 1.577126)
				(mid -0.35208 -0.35208)
				(end 1.577126 -1.32171)
				(width 0.2)
			)
			(gr_arc
				(start -1.422335 1.577126)
				(mid -0.422496 -0.422496)
				(end 1.577126 -1.422335)
				(width 0.2)
			)
			(gr_line
				(start 1.577126 -0.208831)
				(end 1.577126 -1.422335)
				(width 0.2)
			)
			(gr_line
				(start -0.208831 1.577126)
				(end -1.422335 1.577126)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -2.077126 2.077126)
		(size 0.6975 0.6975)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.577126 0.208831)
				(mid 0.422496 -0.422496)
				(end -0.208831 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.310669)
				(mid 0.35208 -0.35208)
				(end -0.310669 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.412325)
				(mid 0.281664 -0.281664)
				(end -0.412325 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.51382)
				(mid 0.211248 -0.211248)
				(end -0.51382 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.615172)
				(mid 0.140832 -0.140832)
				(end -0.615172 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.716397)
				(mid 0.070416 -0.070416)
				(end -0.716397 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.817508)
				(mid 0 0)
				(end -0.817508 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 0.918517)
				(mid -0.070416 0.070416)
				(end -0.918517 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 1.019433)
				(mid -0.140832 0.140832)
				(end -1.019433 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 1.120266)
				(mid -0.211248 0.211248)
				(end -1.120266 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 1.221022)
				(mid -0.281664 0.281664)
				(end -1.221022 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 1.32171)
				(mid -0.35208 0.35208)
				(end -1.32171 -1.577126)
				(width 0.2)
			)
			(gr_arc
				(start 1.577126 1.422335)
				(mid -0.422496 0.422496)
				(end -1.422335 -1.577126)
				(width 0.2)
			)
			(gr_line
				(start -0.208831 -1.577126)
				(end -1.422335 -1.577126)
				(width 0.2)
			)
			(gr_line
				(start 1.577126 0.208831)
				(end 1.577126 1.422335)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 4.4 4.4)
		(drill 4.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 2.077126 -2.077126)
		(size 0.6975 0.6975)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.577126 -0.208831)
				(mid -0.422496 0.422496)
				(end 0.208831 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.310669)
				(mid -0.35208 0.35208)
				(end 0.310669 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.412325)
				(mid -0.281664 0.281664)
				(end 0.412325 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.51382)
				(mid -0.211248 0.211248)
				(end 0.51382 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.615172)
				(mid -0.140832 0.140832)
				(end 0.615172 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.716397)
				(mid -0.070416 0.070416)
				(end 0.716397 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.817508)
				(mid 0 0)
				(end 0.817508 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -0.918517)
				(mid 0.070416 -0.070416)
				(end 0.918517 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -1.019433)
				(mid 0.140832 -0.140832)
				(end 1.019433 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -1.120266)
				(mid 0.211248 -0.211248)
				(end 1.120266 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -1.221022)
				(mid 0.281664 -0.281664)
				(end 1.221022 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -1.32171)
				(mid 0.35208 -0.35208)
				(end 1.32171 1.577126)
				(width 0.2)
			)
			(gr_arc
				(start -1.577126 -1.422335)
				(mid 0.422496 -0.422496)
				(end 1.422335 1.577126)
				(width 0.2)
			)
			(gr_line
				(start 0.208831 1.577126)
				(end 1.422335 1.577126)
				(width 0.2)
			)
			(gr_line
				(start -1.577126 -0.208831)
				(end -1.577126 -1.422335)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 2.077126 2.077126)
		(size 0.6975 0.6975)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.208831 -1.577126)
				(mid -0.422496 -0.422496)
				(end -1.577126 0.208831)
				(width 0.2)
			)
			(gr_arc
				(start 0.310669 -1.577126)
				(mid -0.35208 -0.35208)
				(end -1.577126 0.310669)
				(width 0.2)
			)
			(gr_arc
				(start 0.412325 -1.577126)
				(mid -0.281664 -0.281664)
				(end -1.577126 0.412325)
				(width 0.2)
			)
			(gr_arc
				(start 0.51382 -1.577126)
				(mid -0.211248 -0.211248)
				(end -1.577126 0.51382)
				(width 0.2)
			)
			(gr_arc
				(start 0.615172 -1.577126)
				(mid -0.140832 -0.140832)
				(end -1.577126 0.615172)
				(width 0.2)
			)
			(gr_arc
				(start 0.716397 -1.577126)
				(mid -0.070416 -0.070416)
				(end -1.577126 0.716397)
				(width 0.2)
			)
			(gr_arc
				(start 0.817508 -1.577126)
				(mid 0 0)
				(end -1.577126 0.817508)
				(width 0.2)
			)
			(gr_arc
				(start 0.918517 -1.577126)
				(mid 0.070416 0.070416)
				(end -1.577126 0.918517)
				(width 0.2)
			)
			(gr_arc
				(start 1.019433 -1.577126)
				(mid 0.140832 0.140832)
				(end -1.577126 1.019433)
				(width 0.2)
			)
			(gr_arc
				(start 1.120266 -1.577126)
				(mid 0.211248 0.211248)
				(end -1.577126 1.120266)
				(width 0.2)
			)
			(gr_arc
				(start 1.221022 -1.577126)
				(mid 0.281664 0.281664)
				(end -1.577126 1.221022)
				(width 0.2)
			)
			(gr_arc
				(start 1.32171 -1.577126)
				(mid 0.35208 0.35208)
				(end -1.577126 1.32171)
				(width 0.2)
			)
			(gr_arc
				(start 1.422335 -1.577126)
				(mid 0.422496 0.422496)
				(end -1.577126 1.422335)
				(width 0.2)
			)
			(gr_line
				(start -1.577126 0.208831)
				(end -1.577126 1.422335)
				(width 0.2)
			)
			(gr_line
				(start 0.208831 -1.577126)
				(end 1.422335 -1.577126)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.95 0)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.95)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.95)
		(size 0.992 0.992)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.95 0)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.95 0)
				(end 0 0)
				(width 1.5)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMSSR-3.3mm_H10mm_SnapRivet_9776100960.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
