(footprint "Mounting_Wuerth_WA-SMST-2.25mm_H4mm_9774040943"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole 2.25mm, height 4, Wuerth electronics 9774040943 (https://katalog.we-online.de/em/datasheet/9774040943.pdf), generated with kicad-footprint-generator")
	(tags "Mounting 2.25mm 9774040943")
	(property "Reference" "REF**"
		(at 0 -3.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMST-2.25mm_H4mm_9774040943"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.453104 -1.453104)
		(size 0.505 0.505)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.147677 1.053104)
				(mid 0.286378 0.286378)
				(end 1.053104 -0.147677)
				(width 0.2)
			)
			(gr_arc
				(start -0.240295 1.053104)
				(mid 0.222739 0.222739)
				(end 1.053104 -0.240295)
				(width 0.2)
			)
			(gr_arc
				(start -0.332645 1.053104)
				(mid 0.159099 0.159099)
				(end 1.053104 -0.332645)
				(width 0.2)
			)
			(gr_arc
				(start -0.424767 1.053104)
				(mid 0.095459 0.095459)
				(end 1.053104 -0.424767)
				(width 0.2)
			)
			(gr_arc
				(start -0.516693 1.053104)
				(mid 0.03182 0.03182)
				(end 1.053104 -0.516693)
				(width 0.2)
			)
			(gr_arc
				(start -0.608448 1.053104)
				(mid -0.03182 -0.03182)
				(end 1.053104 -0.608448)
				(width 0.2)
			)
			(gr_arc
				(start -0.700056 1.053104)
				(mid -0.095459 -0.095459)
				(end 1.053104 -0.700056)
				(width 0.2)
			)
			(gr_arc
				(start -0.791534 1.053104)
				(mid -0.159099 -0.159099)
				(end 1.053104 -0.791534)
				(width 0.2)
			)
			(gr_arc
				(start -0.882896 1.053104)
				(mid -0.222739 -0.222739)
				(end 1.053104 -0.882896)
				(width 0.2)
			)
			(gr_arc
				(start -0.974157 1.053104)
				(mid -0.286378 -0.286378)
				(end 1.053104 -0.974157)
				(width 0.2)
			)
			(gr_line
				(start 1.053104 -0.147677)
				(end 1.053104 -0.974157)
				(width 0.2)
			)
			(gr_line
				(start -0.147677 1.053104)
				(end -0.974157 1.053104)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -1.453104 1.453104)
		(size 0.505 0.505)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.053104 0.147677)
				(mid 0.286378 -0.286378)
				(end -0.147677 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.240295)
				(mid 0.222739 -0.222739)
				(end -0.240295 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.332645)
				(mid 0.159099 -0.159099)
				(end -0.332645 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.424767)
				(mid 0.095459 -0.095459)
				(end -0.424767 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.516693)
				(mid 0.03182 -0.03182)
				(end -0.516693 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.608448)
				(mid -0.03182 0.03182)
				(end -0.608448 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.700056)
				(mid -0.095459 0.095459)
				(end -0.700056 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.791534)
				(mid -0.159099 0.159099)
				(end -0.791534 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.882896)
				(mid -0.222739 0.222739)
				(end -0.882896 -1.053104)
				(width 0.2)
			)
			(gr_arc
				(start 1.053104 0.974157)
				(mid -0.286378 0.286378)
				(end -0.974157 -1.053104)
				(width 0.2)
			)
			(gr_line
				(start -0.147677 -1.053104)
				(end -0.974157 -1.053104)
				(width 0.2)
			)
			(gr_line
				(start 1.053104 0.147677)
				(end 1.053104 0.974157)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 1.453104 -1.453104)
		(size 0.505 0.505)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.053104 -0.147677)
				(mid -0.286378 0.286378)
				(end 0.147677 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.240295)
				(mid -0.222739 0.222739)
				(end 0.240295 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.332645)
				(mid -0.159099 0.159099)
				(end 0.332645 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.424767)
				(mid -0.095459 0.095459)
				(end 0.424767 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.516693)
				(mid -0.03182 0.03182)
				(end 0.516693 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.608448)
				(mid 0.03182 -0.03182)
				(end 0.608448 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.700056)
				(mid 0.095459 -0.095459)
				(end 0.700056 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.791534)
				(mid 0.159099 -0.159099)
				(end 0.791534 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.882896)
				(mid 0.222739 -0.222739)
				(end 0.882896 1.053104)
				(width 0.2)
			)
			(gr_arc
				(start -1.053104 -0.974157)
				(mid 0.286378 -0.286378)
				(end 0.974157 1.053104)
				(width 0.2)
			)
			(gr_line
				(start 0.147677 1.053104)
				(end 0.974157 1.053104)
				(width 0.2)
			)
			(gr_line
				(start -1.053104 -0.147677)
				(end -1.053104 -0.974157)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.453104 1.453104)
		(size 0.505 0.505)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.147677 -1.053104)
				(mid -0.286378 -0.286378)
				(end -1.053104 0.147677)
				(width 0.2)
			)
			(gr_arc
				(start 0.240295 -1.053104)
				(mid -0.222739 -0.222739)
				(end -1.053104 0.240295)
				(width 0.2)
			)
			(gr_arc
				(start 0.332645 -1.053104)
				(mid -0.159099 -0.159099)
				(end -1.053104 0.332645)
				(width 0.2)
			)
			(gr_arc
				(start 0.424767 -1.053104)
				(mid -0.095459 -0.095459)
				(end -1.053104 0.424767)
				(width 0.2)
			)
			(gr_arc
				(start 0.516693 -1.053104)
				(mid -0.03182 -0.03182)
				(end -1.053104 0.516693)
				(width 0.2)
			)
			(gr_arc
				(start 0.608448 -1.053104)
				(mid 0.03182 0.03182)
				(end -1.053104 0.608448)
				(width 0.2)
			)
			(gr_arc
				(start 0.700056 -1.053104)
				(mid 0.095459 0.095459)
				(end -1.053104 0.700056)
				(width 0.2)
			)
			(gr_arc
				(start 0.791534 -1.053104)
				(mid 0.159099 0.159099)
				(end -1.053104 0.791534)
				(width 0.2)
			)
			(gr_arc
				(start 0.882896 -1.053104)
				(mid 0.222739 0.222739)
				(end -1.053104 0.882896)
				(width 0.2)
			)
			(gr_arc
				(start 0.974157 -1.053104)
				(mid 0.286378 0.286378)
				(end -1.053104 0.974157)
				(width 0.2)
			)
			(gr_line
				(start -1.053104 0.147677)
				(end -1.053104 0.974157)
				(width 0.2)
			)
			(gr_line
				(start 0.147677 -1.053104)
				(end 0.974157 -1.053104)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.075 0)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.075)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.075)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.075 0)
		(size 1.15 1.15)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.075 0)
				(end 0 0)
				(width 1.15)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMST-2.25mm_H4mm_9774040943.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
