(footprint "Mounting_Wuerth_WA-SMST-2.7mm_H3mm_9774030951"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole 2.7mm, height 3, Wuerth electronics 9774030951 (https://katalog.we-online.de/em/datasheet/9774030951.pdf), generated with kicad-footprint-generator")
	(tags "Mounting 2.7mm 9774030951")
	(property "Reference" "REF**"
		(at 0 -3.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WA-SMST-2.7mm_H3mm_9774030951"
		(at 0 3.95 0)
		(layer "F.Fab")
	)
	(attr smd allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -1.704127 -1.704127)
		(size 0.51 0.51)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -0.250195 1.279127)
				(mid 0.289914 0.289914)
				(end 1.279127 -0.250195)
				(width 0.2)
			)
			(gr_arc
				(start -0.34334 1.279127)
				(mid 0.225488 0.225488)
				(end 1.279127 -0.34334)
				(width 0.2)
			)
			(gr_arc
				(start -0.436309 1.279127)
				(mid 0.161063 0.161063)
				(end 1.279127 -0.436309)
				(width 0.2)
			)
			(gr_arc
				(start -0.529126 1.279127)
				(mid 0.096638 0.096638)
				(end 1.279127 -0.529126)
				(width 0.2)
			)
			(gr_arc
				(start -0.621807 1.279127)
				(mid 0.032213 0.032213)
				(end 1.279127 -0.621807)
				(width 0.2)
			)
			(gr_arc
				(start -0.71437 1.279127)
				(mid -0.032213 -0.032213)
				(end 1.279127 -0.71437)
				(width 0.2)
			)
			(gr_arc
				(start -0.806826 1.279127)
				(mid -0.096638 -0.096638)
				(end 1.279127 -0.806826)
				(width 0.2)
			)
			(gr_arc
				(start -0.899187 1.279127)
				(mid -0.161063 -0.161063)
				(end 1.279127 -0.899187)
				(width 0.2)
			)
			(gr_arc
				(start -0.991463 1.279127)
				(mid -0.225488 -0.225488)
				(end 1.279127 -0.991463)
				(width 0.2)
			)
			(gr_arc
				(start -1.083663 1.279127)
				(mid -0.289914 -0.289914)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 -0.250195)
				(end 1.279127 -1.083663)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 1.279127)
				(end -1.083663 1.279127)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at -1.704127 1.704127)
		(size 0.51 0.51)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 1.279127 0.250195)
				(mid 0.289914 -0.289914)
				(end -0.250195 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.34334)
				(mid 0.225488 -0.225488)
				(end -0.34334 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.436309)
				(mid 0.161063 -0.161063)
				(end -0.436309 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.529126)
				(mid 0.096638 -0.096638)
				(end -0.529126 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.621807)
				(mid 0.032213 -0.032213)
				(end -0.621807 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.71437)
				(mid -0.032213 0.032213)
				(end -0.71437 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.806826)
				(mid -0.096638 0.096638)
				(end -0.806826 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.899187)
				(mid -0.161063 0.161063)
				(end -0.899187 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 0.991463)
				(mid -0.225488 0.225488)
				(end -0.991463 -1.279127)
				(width 0.2)
			)
			(gr_arc
				(start 1.279127 1.083663)
				(mid -0.289914 0.289914)
				(end -1.083663 -1.279127)
				(width 0.2)
			)
			(gr_line
				(start -0.250195 -1.279127)
				(end -1.083663 -1.279127)
				(width 0.2)
			)
			(gr_line
				(start 1.279127 0.250195)
				(end 1.279127 1.083663)
				(width 0.2)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 3.7 3.7)
		(drill 3.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd custom
		(at 1.704127 -1.704127)
		(size 0.51 0.51)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start -1.279127 -0.250195)
				(mid -0.289914 0.289914)
				(end 0.250195 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.34334)
				(mid -0.225488 0.225488)
				(end 0.34334 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.436309)
				(mid -0.161063 0.161063)
				(end 0.436309 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.529126)
				(mid -0.096638 0.096638)
				(end 0.529126 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.621807)
				(mid -0.032213 0.032213)
				(end 0.621807 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.71437)
				(mid 0.032213 -0.032213)
				(end 0.71437 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.806826)
				(mid 0.096638 -0.096638)
				(end 0.806826 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.899187)
				(mid 0.161063 -0.161063)
				(end 0.899187 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -0.991463)
				(mid 0.225488 -0.225488)
				(end 0.991463 1.279127)
				(width 0.2)
			)
			(gr_arc
				(start -1.279127 -1.083663)
				(mid 0.289914 -0.289914)
				(end 1.083663 1.279127)
				(width 0.2)
			)
			(gr_line
				(start 0.250195 1.279127)
				(end 1.083663 1.279127)
				(width 0.2)
			)
			(gr_line
				(start -1.279127 -0.250195)
				(end -1.279127 -1.083663)
				(width 0.2)
			)
		)
	)
	(pad "" smd custom
		(at 1.704127 1.704127)
		(size 0.51 0.51)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_arc
				(start 0.250195 -1.279127)
				(mid -0.289914 -0.289914)
				(end -1.279127 0.250195)
				(width 0.2)
			)
			(gr_arc
				(start 0.34334 -1.279127)
				(mid -0.225488 -0.225488)
				(end -1.279127 0.34334)
				(width 0.2)
			)
			(gr_arc
				(start 0.436309 -1.279127)
				(mid -0.161063 -0.161063)
				(end -1.279127 0.436309)
				(width 0.2)
			)
			(gr_arc
				(start 0.529126 -1.279127)
				(mid -0.096638 -0.096638)
				(end -1.279127 0.529126)
				(width 0.2)
			)
			(gr_arc
				(start 0.621807 -1.279127)
				(mid -0.032213 -0.032213)
				(end -1.279127 0.621807)
				(width 0.2)
			)
			(gr_arc
				(start 0.71437 -1.279127)
				(mid 0.032213 0.032213)
				(end -1.279127 0.71437)
				(width 0.2)
			)
			(gr_arc
				(start 0.806826 -1.279127)
				(mid 0.096638 0.096638)
				(end -1.279127 0.806826)
				(width 0.2)
			)
			(gr_arc
				(start 0.899187 -1.279127)
				(mid 0.161063 0.161063)
				(end -1.279127 0.899187)
				(width 0.2)
			)
			(gr_arc
				(start 0.991463 -1.279127)
				(mid 0.225488 0.225488)
				(end -1.279127 0.991463)
				(width 0.2)
			)
			(gr_arc
				(start 1.083663 -1.279127)
				(mid 0.289914 0.289914)
				(end -1.279127 1.083663)
				(width 0.2)
			)
			(gr_line
				(start -1.279127 0.250195)
				(end -1.279127 1.083663)
				(width 0.2)
			)
			(gr_line
				(start 0.250195 -1.279127)
				(end 1.083663 -1.279127)
				(width 0.2)
			)
		)
	)
	(pad "1" smd circle
		(at -2.425 0)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 -2.425)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd circle
		(at 0 2.425)
		(size 0.642 0.642)
		(layers "F.Cu")
	)
	(pad "1" smd custom
		(at 2.425 0)
		(size 1.15 1.15)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center -2.425 0)
				(end 0 0)
				(width 1.15)
			)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WA-SMST-2.7mm_H3mm_9774030951.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
