(footprint "Mounting_Wuerth_WP-SMRA-M3_L7mm_7466303_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Right-angle SMD mounting Hardware, inside threaded M3, length 7m, total height 5mm, Würth electronics 7466303 (https://www.we-online.com/components/products/datasheet/7466303.pdf)")
	(tags "threaded screw")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Mounting_Wuerth_WP-SMRA-M3_L7mm_7466303_Horizontal"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.6 -1.35)
		(size 2.95 2.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1020408163)
		(solder_paste_margin -0.1)
	)
	(pad "1" smd roundrect
		(at -1.6 1.35)
		(size 2.95 2.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1020408163)
		(solder_paste_margin -0.1)
	)
	(pad "1" smd roundrect
		(at 1.6 -1.35)
		(size 2.95 2.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1020408163)
		(solder_paste_margin -0.1)
	)
	(pad "1" smd roundrect
		(at 1.6 1.35)
		(size 2.95 2.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1020408163)
		(solder_paste_margin -0.1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Mounting_Wuerth.3dshapes/Mounting_Wuerth_WP-SMRA-M3_L7mm_7466303_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
