(footprint "ADNS-9800"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Laser Gaming Sensor ADNS-9800")
	(tags "MOUSE MOUSE_SENSOR LASER_GAMING_SENSOR")
	(property "Reference" "REF**"
		(at 3 -2.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "ADNS-9800"
		(at 6.5 15.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start 1.7 -0.5)
		(end 10.9 -0.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.7 12.96)
		(end 1.7 -0.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.9 -0.5)
		(end 10.9 12.96)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.9 12.96)
		(end 1.7 12.96)
		(layer "Edge.Cuts")
	)
	(fp_text user "Optical Center"
		(at 6.25 6.25 180)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 6.3 7.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 1.78)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 3.56)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 5.34)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 7.12)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 8.9)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 10.68)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 12.46)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 12.6 12.46)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 12.6 10.68)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 12.6 8.9)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 12.6 7.12)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 12.6 5.34)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 12.6 3.56)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 12.6 1.78)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 12.6 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/OptoDevice.3dshapes/ADNS-9800.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
